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Товарлардын келип чыгышын сертификаттоо жана верификациялоонун электрондук системасынын алкагында бир тараптан Евразия экономикалык бирлиги жана ага мүчө мамлекеттер менен экинчи тараптан Вьетнам Социалисттик Республикасынын ортосунда электрондук маалымат алмашуу жөнүндө протоколго кол коюу маселелери жөнүндө

2014-жылдын 29-майындагы Евразия экономикалык бирлиги жөнүндө келишимдин 7-беренесинин 2-пунктунун биринчи абзацын, 
2018-жылдын 14-майындагы Евразия экономикалык бирлигинин үчүнчү мамлекеттер, эл аралык уюмдар же эл аралык интеграциялык бирикмелер менен эл аралык келишимдери жөнүндө Макулдашуунун 10-беренесин жана Евразия экономикалык комиссиясы жөнүндө жобонун (2014-жылдын 29-майындагы Евразия экономикалык бирлиги жөнүндө келишимге № 1 тиркеме) 6-пунктун жетекчиликке алып, Жогорку Евразия экономикалык кеңеши чечти:
1. Товарлардын келип чыгышын сертификаттоо жана верификациялоонун электрондук системасынын алкагында бир тараптан Евразия экономикалык бирлиги жана ага мүчө мамлекеттер менен экинчи тараптан Вьетнам Социалисттик Республикасынын ортосунда электрондук маалымат алмашуу жөнүндө протоколдун долбоору (тиркелет) жактырылсын
2. Евразия экономикалык комиссиясынын соода боюнча Коллегия мүчөсү (министр) А.А. Слепневге Евразия экономикалык бирлигинин мүчө мамлекеттери зарыл болгон мамлекеттик ички жол-жоболорду аяктагандан кийин Евразия экономикалык бирлигинин атынан ушул чечимдин 
1-пунктунда көрсөтүлгөн протоколго кол коюу тапшырылсын, зарыл болгон учурда тиркелген долбоорго принциптүү мүнөзгө ээ болбогон өзгөртүүлөрдү киргизүүгө уруксат берилсин.
3. Бул Чечим расмий жарыяланган датадан тартып күчүнө кирет. 

Жогорку Евразия экономикалык кеңешинин мүчөлөрү:

	Армения Республикасы-
нан
	Беларусь Республикасы-
нан
	Казакстан Республикасы-
нан
	Кыргыз Республикасы-
нан
	Россия Федерациясы-нан
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P R O T O C O L
on electronic information exchange between the Eurasian Economic Union and its Member States, of the one part, and the Socialist Republic of Viet Nam, of the other part, within the Electronic Origin Certification and Verification System
	
The Governments of the Member States of the Eurasian Economic Union (hereinafter referred to as “the EAEU Member States”) and the Eurasian Economic Union, of the one part, and the Government of the Socialist Republic of Viet Nam (hereinafter referred to as “Viet Nam”), of the other part (hereinafter referred to as “the Parties”):

Recalling Article 4.29 (Development and Implementation of Electronic Origin Certification and Verification System) of the Free Trade Agreement between the Eurasian Economic Union and its Member States, of the one part, and  the Socialist Republic of Viet Nam, of the other part, on 29 May 2015;

Welcoming the reduction of the costs relating to the documentary proof of origin used for the purposes of application of tariff preferences;

Aiming at simplifying the procedures and reducing the time for the application
of tariff preferences; and

Desiring to strengthen cooperation between the customs authorities and the bodies and organisations authorised to issue certificates of origin of the Parties,

HAVE AGREED as follows:

Article 1
Definitions

For the purposes of this Protocol:

“Authorised Body” means a body or an organisation authorised by the EAEU Member State or by Viet Nam to issue a certificate of origin, generate and maintain information resources containing information on issued certificates of origin, and to provide information on certificates of origin, for their verification in response to the requests of the customs authorities; 

“Integrated information system of the EAEU” means a set of geographically distributed state information resources and information systems of authorised authorities, information resources and information systems of the Eurasian Economic Commission, combined by the national segments of the EAEU Member States and the integration segment of the Eurasian Economic Commission; and
“National Single Window of Viet Nam” means the mechanism of Viet Nam which allows the customs declarants to send the information and electronic documents for completion of customs procedures and procedures of state management agencies related to exported and imported goods through an integrated information system.

Article 2
Transmission of Information

1. For the purpose of this Article, the exchange of information shall be carried out via the Integrated Information System of the EAEU and the National Single Window of Viet Nam based on the requirements of the Technical Specifications specified in the Annex to this Protocol.
2. The Authorised Body of Viet Nam shall transmit to the relevant central
customs authority of the EAEU Member States the information contained in the certificates of origin issued for goods exported from the territory of Viet Nam to the territory of this EAEU Member State.
3. The relevant Authorised Body of the EAEU Member State shall transmit to the central customs authority of Viet Nam the information contained in the certificates of origin issued for goods exported from the territory of this EAEU Member State to the territory of Viet Nam.

Article 3
Confidentiality

All information provided in accordance with this Protocol shall be treated by the Parties as confidential in accordance with their respective domestic laws and regulations. It shall not be disclosed by the customs authorities of a Party without the written permission of the Authorised Bodies of the other Party which provided such information except to the extent that it may be required to be disclosed in the context of judicial proceedings.



Article 4
Amendments
1. This Protocol may be amended by mutual consent of the Parties.
2. Such amendments shall be formalised by separate protocols and constitute an integral part of this Protocol.

Article 5
Consultations

1. Any matters related to the implementation of this Protocol shall be settled through consultations or negotiations between the Parties.
2. If a Party considers that the matter cannot be settled through consultations or negotiations as provided for in paragraph 1 of this Article, that Party shall have the right to seek resolution in the Joint Committee established in accordance with Article 1.4 (Joint Committee) of the Free Trade Agreement between the Eurasian Economic Union and its Member States, of the one part, and the Socialist Republic of Viet Nam, of the other part, on 29 May 2015.

Article 6
Entry into Force

1. This Protocol shall enter into force on the date of receipt, through diplomatic channels, of the last written notification certifying that the Parties have completed their respective internal legal procedures necessary for entry into force of this Protocol.
2. The exchange of notifications provided for in paragraph 1 of this Article shall be performed by Viet Nam and the Eurasian Economic Commission as the custodian of this Protocol authorised by the Republic of Armenia, the Republic of Belarus, the Republic of Kazakhstan, the Kyrgyz Republic and the Russian Federation.

DONE at				, this 			day of 		20____,
in two originals in the English language, both texts being equally authentic.




	For the Government 
of the Republic of Armenia
	For the Government
of the Socialist Republic 
of Viet Nam






For the Government
of the Republic of Belarus





For the Government
of the Republic of Kazakhstan





For the Cabinet of Ministers
of the Kyrgyz Republic





For the Government
of the Russian Federation





For the Eurasian Economic Union






Annex
to the Protocol on electronic information exchange between the Eurasian Economic Union and its Member States, of the one part, and the Socialist Republic of Viet Nam, of the other part, within the Electronic Origin Certification and Verification System




T E C H N I C A L S P E C I F I C A T I O N

Pages 118


I. Purpose of the document
These Technical Specifications set technical requirements and conditions for the implementation of the electronic information exchange between the central customs authorities of the Member States of the Eurasian Economic Union (hereinafter referred to as «the Member States», «the Union») and of the Socialist Republic of Viet Nam within the Electronic Origin Certification and Verification System (hereinafter referred to as «the Parties», «the EOCVS») in accordance with Article 4.29 of the Free Trade Agreement between the Eurasian Economic Union and its Member States, of the one part, and the Socialist Republic of Viet Nam, of the other part, dated May 29, 2015 (hereinafter referred to as «the Agreement»).
These Technical Specifications define participants, procedures and regulations of the electronic information exchange, content and structure of transmitted information and messages, used classifiers and directories, security requirements for information exchange and technical aspects and interaction parameters within the EOCVS for exchanging information on certificates of origin issued by the authorized bodies of one Party and used by the customs authorities of the other Party in order to verify validity and content of the issued certificates of origin.


II. Chronology of the documentʼs revisions

	Number of revision
	Date of revision
	Description of the changes
	Initiator of the changes

	01.00
	24.09.2017
	First version of the document
	Eurasian Economic
Commission

	15.7
	13.12.2017
	Draft for 3th round of negotiations
	Eurasian Economic
Commission

	15.8
	21.12.2017
	Results of 3th round of 
negotiations are implemented

	Joint working group

	15.10
	28.02.2018
	Comments and proposals of
Vietnamese Side are implemented
	Joint working group


	15.11
	02.03.2018
	The results of negotiations on exchange of customs information 
are included
	Eurasian Economic
Commission

	16.00
	01.09.2021
	The results of negotiations reached during the Subcommittee Meeting on Rules of Origin in December 
2019 are included
	Eurasian Economic
Commission

	17.00
	13.11.2023
	The results of negotiations reached during the fifth session of the Joint Committee in November 2023 are included
	Eurasian Economic
Commission





III.Terms and abbreviations

The following terms and definitions are used in these Technical Specification:
«SOAP» (Simple Object Access Protocol) – message-exchange protocol in the distributed computing environment;
«UML» – Unified Modeling Language;
«UUID» – Universally Unique Identifier;
«XML» (Extensible Markup Language) – recommended by the World Wide Web Consortium (W3C) Extensible Markup Language;
«Asynchronous Interaction» – a kind of electronic data exchange, in which the Sender resumes his work immediately after sending the message, without waiting for a response from the receiver;
«Business process» – a set of interrelated operations and procedures for implementation of the electronic information exchange;
«Verification» – the procedure for confirming the authenticity of the certificate of origin;
«External Gateway» – a subsystem of the Integrated information system of the Union that provides interaction with the National Single Window of Viet Nam;
«Information Protection» – development and implementation of a set of legal, organizational and technical measures to identify, achieve and maintain the confidentiality, integrity and availability of information and processing facilities in order to eliminate or minimize unacceptable risks for the participants of information exchange;
«Initiator» – a participant of electronic information exchange initiating the transaction;
«Information system» – a set of information technologies and technical means to ensure the processing of information resources;
«Information resource» – an ordered set of documented information (databases, other information arrays) contained in Information Systems; 
«Communication channel» – the unidirectional network connection for transmitting electronic messages;
«Classifier» – a systematic, structured and codified list of names of items of classification;
«Commission» – the Eurasian Economic Commission which is a permanent regulatory body of the Eurasian Economic Union in accordance with the Treaty on the Eurasian Economic Union dated May 29, 2014;
«Integrated information system of the Union» – a set of geographically distributed state information resources and information systems of authorized authorities, information resources and information systems of the Eurasian Economic Commission, combined by the national segments of the Member States of the Eurasian Economic Union and the integration segment of the Eurasian Economic Commission; 
«National Single Window of Viet Nam» – the mechanism which allows customs declarant on the Viet Nam side to send information and electronic documents for performing of customs procedures and procedures of state management agencies related to exported and imported goods, as well as which allows the Authorised Bodies of Viet Nam to receive the information necessary for performing of customs procedures, providing the information exchange with the external gateway of the Integrated information system of the Union;
«Business Process Operation» – a regular, repetitive action, which is part of the range of functions, tasks of a certain Participant of the Business Process;
«Control Error» – a type of exception signals that occurs when the notice received by the Respondent is checked, or the waiting time of the notice that the Respondent accepts the received information for processing expires;
«Business process procedure» – a set of interrelated operations performed by participants of the business process and aimed at solving a specific task within a business process;
«Respondent» – a participant of electronic information exchange exchanging messages with the Initiator within the transaction;
«Service» – the process of providing users with information technology resources to ensure the performance of their business functions, which has the ability to perform the required functions in a given period of time;
«Certificate of origin» – certificate of origin form EAV issued by an authorized body of the Party in accordance with Section 2 of Chapter 4 of the Agreement;
«Message» – a formalised information transmitted from the sender to the receiver using information and telecommunications networks;
«Directory» – a systematic, structured and codified list of information, that is homogeneous in its content or substance;
«Transaction» – an elementary information interaction between two participants of business process, which is carried out by each participant within its Business Process Operation;
«Participant of the business process» – a participant of electronic information exchange within the business process. 
In order to provide clear presentation of transferred information and message structures tables are used. These tables contain the following columns:
«requisite name / element»  – common or official verbal mark of an electronic information requisite or a message element; 
«requisite description / description» –  a text defining the meaning (semantology) of an electronic information requisite or a message element;
«data type» – a verbal mark of possible values of an electronic information requisite or a message element;
«mult.» – requisite multiplicity - necessity (optionality) and the number  possible requisite or message element repetitions.
To indicate the necessity of filling electronic information or message element structure requisites, the following notations are used in «mult.» column:
1 –  a requisite (element) is obligatory, no repetitions are allowed;
n – a requisite (element) is obligatory, shall be repeated n times, n > 1;
0..1 – a requisite (element) is optional, no repetitions are allowed;
0..* – a requisite (element) is optional, can be repeated without restrictions;
0..m – a requisite (element) is optional, can be repeated no more than  m times, m>1;
1..* – a requisite (element) is obligatory, can be repeated without restrictions;
n..* – a requisite (element) is obligatory, shall be repeated at least n times, n > 1;
n..m – a requisite (element) is obligatory, must be repeated at least n times and not more than m times, n >1, m > n.

IV. General information

4.1 General principles of the electronic information exchange

Electronic information exchange within the EOCVS is intended to ensure the possibility to verify authenticity, issuance and content of the issued certificates of origin.
EOCVS is developed to create databases of certificates of origin issued by authorized bodies of exporting countries available for customs authorities of importing countries to verify the issuance and the content of issued certificates of origin.
Information from certificates of origin is exchanged between the participants within the EOCVS on a regular basis by means of electronic messages exchange.
Participants of electronic information exchange ensure the development and maintenance of structured information resources containing current information on certificates of origin, as well as information systems that support services for electronic information exchange.
Requirements for composition and structure of data used in data exchange are defined based on international standards and generally accepted initiatives in the field of electronic data exchange (including the Data Model of the World Customs Organization).
These Technical Specifications do not include requirements for unification of database structures and rules for their organization and functioning. Such requirements are defined at the national level.
Electronic information exchange participants shall protect transmitted information (including protection of information authenticity and integrity), as well as protect information from unauthorised access, destruction, change and prevent inappropriate storage.
Electronic information exchange participants submitting information shall ensure the completeness and correctness of information on issued certificates of origin provided within the EOCVS to enable the participants receiving information to check the issuance of certificates of origin and the authenticity of information contained.
Electronic information exchange participants shall provide 24-hour functioning of information resources and information systems, as well as related services.


4.2. Participants of electronic information exchange
The electronic information exchange involves:
1. Central customs authorities of the Member States and Viet Nam receiving information on the issued certificates of origin for their verification: 
The State Revenue Committee of the Republic of Armenia; 
The State Customs Committee of the Republic of Belarus;
The State Revenue Committee of the Ministry of finance of the Republic of Kazakhstan;
The Customs Service under the Ministry of Finance of the Kyrgyz Republic;
The Federal Customs Service (the Russian Federation);
The Ministry of Finance (General Department of Viet Nam Customs) of the Socialist Republic of Viet Nam.
2. Authorized bodies of the Member States and Viet Nam providing information on certificates of origin:
The Chamber of Commerce and Industry of the Republic of Armenia; 
The Chamber of Commerce and Industry of the Republic of Belarus; 
The National Chamber of Entrepreneurs of the Republic of Kazakhstan; 
The Chamber of Commerce and Industry of the Kyrgyz Republic;
The Chamber of Commerce and Industry of the Russian Federation;
The Ministry of Industry and Trade of the Socialist Republic of Viet Nam.

4.3. The main technical solutions
Electronic information exchange within the EOCVS is carried out by its participants using the Integrated Information System of the Union (hereinafter referred to as «the IIS») and the National Single Window of Viet Nam.
The information transmitted by the authorized bodies of Viet Nam, using the National Single Window of Viet Nam facilities through the External Gateway services is received by the IIS and then it is routed to the central customs authorities of the Member States through the relevant national segments of the Member States.
The information transmitted by the authorized bodies of the Member States through the relevant national segments of the Member States, is transmitted to the IIS, enters the External Gateway and then it is transmitted through the services of the National Single Window of Viet Nam to the customs authorities of Viet Nam. Electronic information exchange within the EOCVS is carried out by its participants at the logic levels, such as transport, technological and application levels.
Procedures of electronic information exchange at the transport level between the External Gateway and the National Single Window of Viet Nam ensure data delivery via HTTP protocol.
Electronic information exchange between the External Gateway and the National Single Window of Viet Nam at the technological level is implemented by means of messages in the SOAP format.
Procedures of electronic information exchange at the application level provide exchanging of electronic data (hereinafter referred to as “the applied data”) between the participants of electronic information exchange through messaging.
Electronic information exchange at the application level is carried out by asynchronous interaction in which the sender resumes his work immediately after sending the message without waiting for the response from the recipient.
The requirements to the structure and format of messages as well as the procedure of messaging at the technological level are established in accordance with Sections VI and VII of these Technical Specifications.

4.4 Requirements for unique identification of information
A unique identifier is assigned to each document in electronic form used within the electronic information exchange.
The following information is used as a unique identifier of the certificate of origin issued by the authorized body of the Party: 
Registration number of the certificate of origin;
Certificate of origin type;
Country of issuance;
Date of certification (issuance of the certificate of origin);
The unique identifier of an electronic message specified in the header block at the technological level is the UUID electronic message identifier as RFC 4122 Specification (http://www.ietf.org/rfc/rfc4122.txt).
Cohesiveness of electronic messages at the technological level is determined by the identifier of cohesive message sent in the header block.
V. Description of business processes of electronic information exchange (information exchange regulations)
5.1. Description of electronic information exchange participants» roles within business process implementation
The roles of business process participants within the EOCVS are listed in Table 1.
Table 1
The list of business process participants» roles
	Designation
	Name
	Description

	ESS.VN.ACT.001
	authorized body-information
owner
	an authorized body of an exporting country which collects, stores and submits current information on certificates of origin to a receiving customs authority

	ESS.VN.ACT.002

	customs authority-information
receiver

	a customs authority of an importing country which receives, processes and stores certificates of origin submitted by authorized owning body



Within the EOCVS the authorized bodies develop and maintain their own information resources containing electronic information on certificates of origin. During business process execution customs authorities-information receivers develop and maintain the information resources containing electronic information about certificates of origin provided by authorized bodies-information owners.
Business process procedures are provided in Table 2.
Table 2.
Business process procedures
	Designation
	Name

	ESS. VN. PRC.001
	providing information on the issued certificate of origin


	ESS. VN. PRC.002
	receiving information on the certificate of origin




Description of the business process structure is shown in Figure 1.
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Figure 1. Business process structure

5.2 Business process procedures

5.2.1.The procedure «Providing information on the issued certificate of origin»
The procedure «Providing information on the issued certificate of origin» shall be carried out within 4 hours after the authorized body-information owner performs one of the following procedures:
issuance of the original certificate of origin;
issuance of the duplicate of certificate of origin;
issuance of the certificate of origin in substitution of the original certificate of origin;
annulment (recall) of the previously issued original certificate of origin, the duplicate of certificate of origin, or the certificate of origin in substitution of the original certificate of origin;
inclusion of information related to it in the information resource containing information about certificates of origin.
The scheme of the procedure “Providing information on the issued certificate of origin” is provided in Figure 2.
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Figure 2. Scheme of the procedure «Providing information on the issued certificate of origin»

The operation «Transferring information on the issued certificate of origin» is carried out first, followed by preparing and providing information on the issued (annulled, recalled) certificate of origin to the receiving customs authority by the authorized owning body.
When the receiving customs authority receives information on the issued (annulled, recalled) certificate of origin, the procedure «Receiving and processing of information on the issued certificate of origin» shall be carried out, followed by receiving, processing and providing notice on the results of processing to the authorized owning body by the receiving customs authority.
When the authorized owning body receives the notice on the results of processing from the receiving customs authority, the procedure «Receiving and processing of the notice on the results of processing of information on the issued certificate» is carried out. Based on the results of this operation, the authorized owning body processes the received notice.
The result of the procedure «Providing information on the issued certificate of origin» is the provision of information on the issued (annulled, recalled) certificate of origin by the authorized owning body and its processing by the receiving customs authority.
The list of operations carried out under the procedure «Providing information on the issued certificate of origin» is given in Table 3.

      Table 3
List of business process operations carried out within the procedure «Providing information on the issued certificate of origin» (ESS.VN.PRC.001)

	Designation
	Name
	Description

	ESS.VN.OPR.001

	transferring information on the issued
certificate of origin

	provided in Table 4


	ESS.VN.OPR.002
	receiving and processing of information on
the issued certificate of origin

	provided in Table 5


	ESS.VN.OPR.003

	receiving and processing of the notice on the results of processing of information on the issued certificate of origin

	provided in Table 6



The description of the operation «Transferring information on the issued certificate of origin» (ESS.VN.OPR.001) is given in Table 4.
Table 4

Description of the operation «Transferring information on the issued certificate of Origin» (ESS.VN.OPR.001 )
	No.

	Element

	Description

	1
	Designation
	ESS.VN.OPR.00l

	2
	Operation

	Transferring of information on the issued certificate of origin

	3
	Executor

	authorized body-information owner

	4
	Execution conditions

	carried out within 4 hours after the certificate of origin is issued (annulled, recalled), and the executor includes information on it into the information resource

	5
	Restrictions

	the format and structure of the information provided shall be in accordance with the description provided in Appendix В

	6
	Operation description
	the executor prepares information on the issued (annulled, recalled) certificate of origin and provides the receiving customs authority with it

	7
	Results

	information on the issued (annulled, recalled) certificate of origin is prepared and transferred to the receiving customs authority




The description of the operation «Receiving and processing of information on the issued certificate of origin» (ESS.VN.OPR.002) is given in Table 5.
   Table 5
Description of the operation «Receiving and processing of information on the issued certificate of origin» (ESS.VN.OPR.002)

	No.

	Element

	Description

	1
	Designation
	ESS.VN.OPR.002

	2
	Operation

	receiving and processing of information on the issued
certificate of origin

	3
	Executor

	customs authority-information receiver

	4
	Execution conditions

	carried out after the executor receives information on the issued (annulled, recalled) certificate of origin (the operation «Transferring i nformation on the issued certificate of origin»
(ESS.VN.OPR.OOl ))

	5
	Restrictions

	the format and structure of provided information shall
comply with the description provided in Appendix В

	6
	Operation description

	the executor receives and checks information on the issued (annulled, recalled) certificate of origin and provides the authorized owning body with the notice on the results of information processing

	7
	Results
	information on the issued (annulled, recalled) certificate of origin is processed, and the authorized owning body is provided with the notice on the results



The description of the operation «Receiving and processing of the notice on the results of processing of information on the issued certificate of origin» (ESS.VN.OPR.003) is given in Table 6.

 Table 6
Description of the operation «Receiving and processing of the notice on the results of processing of information on the issued certificate of origin» (ESS.VN.OPR.003)

	№.
	Element
	Description

	1
	Designation

	ESS.VN.OPR.003


	2
	Operation

	receiving and processing of the notice on the results of
processing of information on the issued certificate of origin

	3
	Executor
	authorized body-information owner

	4
	Execution conditions

	carried out after the executor receives the notice on the results of processing of information (the operation «Receiving and processing of information on the issued certificate of origin» (ESS.VN.OPR.002))

	5
	Restrictions

	the format and structure of the information provided shall be in accordance with the description provided in Appendix В

	6
	Operation description
	he executor receives and processes the notice on the results
of processing of information on the issued (annulled,
recalled) certificate of origin

	7
	Results

	the notice on the results of processing of information is
processed



5.2.2. The procedure «Receiving information on the certificate of origin»
If necessary the receiving customs authority can generate a request to confirm the authenticity of a certain certificate of origin. The scheme of the procedure «Receiving information about the certificate of origin» is given in Figure 3.
The procedure «Receiving information on the certificate of origin» is carried out by the receiving customs authority upon the request, if the information on the issued certificate of origin is necessary. The authorized body-information owner, having received such a request, generates the response containing the requested data or information about their absence.
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Figure 3. Scheme of the procedure «Receiving information on the certificate of origin»
The operation «Requesting information about the certificate of origin» is carried out first, according to the results of which the customs recipient body forms and sends to the authorized authority-owner of the information request to provide information about the certificate of origin.
When the request for providing information on the certificate of origin is received by the authorized owning body, the operation «Providing information on the certificate of origin» is carried out, based on the results of which the authorized owning body generates and sends current information on the certificate of origin or notice on absence of information complying with the parameters of the request to the receiving customs authority.
When the receiving customs authority receives current information on the certificate of origin or the notice on absence of information complying with the parameters of request, the operation «Receiving and processing of information on the certificate of origin» is carried out, followed by the processing of received information by the receiving customs authority.
The result of the procedure «Receiving information on the certificate of origin» is the receiving and processing of current information on the certain certificate of origin or notice on the absence of information complying with the request parameters by the receiving customs authority.
The list of business process operations carried out within the procedure «Receiving information on the certificate of origin» (ESS.VN.PRC.002) is given in   Table 7. 
   Table 7
List of business process operations carried out within the procedure «Receiving information on the certificate of origin» (ESS.VN.PRC.002)

	
Designation

	
Name
	
Description

	ESS.VN.OPR.004
	requesting for information about the certificate of origin
	provided in Table 8

	ESS.VN.OPR.005
	providing information about certificate of origin
	provided in Table 9

	ESS.VN.OPR.006


	receiving and processing of information on the certificate of origin
	provided in Table 10



The description of the operation «Requesting for information on the certificate of origin» (ESS.VN.OPR.004) is given in Table 8.
   Table 8

Description of the operation «Requesting for information on the certificate of origin» (ESS.VN.OPR.004)

	No
	Element
	Description

	1
	Designation

	ESS.VN.OPR.004


	2
	Operation
	requesting for information on the certificate of origin


	3
	Executor

	customs authority-information receiver

	4
	Execution conditions

	performed if necessary to receive information about the certificate of origin by the customs authority- information receiver

	5
	Restrictions

	the format and structure of the request shall be in
accordance with the description given in Appendix В


	6
	Operation description

	the executor generates and sends a request for providing information about the certificate of origin to the authorized body-information owner


	7
	Results

	the request for providing information about the certificate of origin is sent to the authorized body- information owner




The description of the operation «Providing information on the certificate of origin» (ESS.VN.OPR.005) is given in Table 9.
Table 9
Description of the operation «Providing information on the certificate of origin» (ESS.VN.OPR.005)

	No.
	Element
	Description

	1
	Designation
	ESS.VN.OPR.005

	2
	Operation
	providing information on the certificate of origin

	3
	Executor
	authorized body-information owner

	4
	Execution conditions
	carried out after the request for providing information
on the certificate of origin (the operation «Requesting for information on the certificate of origin» (ESS.VN.OPR.004)) is received

	5
	Restrictions
	the format and structure of the request and the provided information shall be in accordance with the description given in Appendix В

	6
	Operation description

	the executor checks the received request, generates and sends current information on the certificate of origin or the notice on absence of information complying with the request parameters, indicating the code of the processing result, corresponding to the absence of information, to the receiving customs authority

	7
	Results
	information on the certificate of origin or the notice on absence of information complying with the request parameters is provided to the receiving customs authority



The description of the operation «Receiving and processing of information on the certificate of origin» (ESS.VN.OPR.006) is given in Table 10.
Table 10
Description of the operation «Receiving and processing of information on the certificate of origin» (ESS.VN.OPR.006)
	No.

	Element

	Designation

	1
	Description
	ESS.VN.OPR.006

	2
	Operation

	receiving and processing of information on the certificate of origin

	3
	Executor
	customs authority-information receiver

	4
	Execution conditions
	carried out after information on the certificate of origin or notice on the absence of information complying with the request parameters (the operation “Providing information on the certificate of origin” (ESS.VN.OPR.005)) is provided

	5
	Restrictions

	the format and structure of the provided information shall be in accordance with the description given in Appendix В

	6
	Operation description
	the executor processes the received information

	7
	Results

	the information about the certificate of origin or the notification on absence of information complying with the parameters of the request is received and processed



5.3. Regulation of interaction during the implementation of the business process
Information interaction of participants during the implementation of thebusiness process is carried out through transactions.
Information interaction defines the order of execution of transactions. Each transaction is the exchange of messages between the participants of electronic information exchange in order to synchronize the statuses of information resources containing information on certificates of origin. For each information interaction, the relationships between operations and the corresponding transactions are defined.
Within the operation (the initiating operation) one participant of the electronic information exchange (the initiator) shall provide another participant of electronic information exchange (the respondent) with a message, in response to which the respondent shall send a response message within the operation he performs (the receiving operation).
Messages exchanged within the business process shall be formed in accordance with the requirements specified in Section VI of these Technical specifications.
Table 11 presents a relationship between the operations, intermediate and resulting states of information objects of business process and transactions for each Business Process Procedure. 
                             Table 11
The list of transactions
	No.
	Operation performed by the Initiator
	Intermediate state of information object of the business process
	Operation performed by the Respondent

	Resulting state of information object of the business process
	Transaction


	1
	Providing information on the issued certificate of origin (ESS.VN.PRC.001)

	1.1
	transferring information on the issued certificate of origin (ESS.VN.OPR.001)receiving and processing of the notice on the results of processing of infonnation on the issued certificate of origin (ESS.VN.OPR.003)
	certificates of origin
(ESS.VN.BEN.001):
information on the issued certificate of origin is transferred

	receiving and processing of information on the issued certificate of origin (ESS.VN.OPR.002)
	certificates of origin
(ESS.VN.BEN.001):
information on the issued certificate of origin is received

	providing information on the issued certificate of origin (ESS.VN.TRN.001)

	2

	Receiving information on the certificate of origin (ESS.VN.PRC.002)

	2.1

	requesting for information on the certificate of origin (ESS.VN.OPR.004)
receiving and processing of information on the certificate  of origin (ESS.VN.OPR.006)

	certificates of origin
(ESS.VN.BEN.001):
information on the issued certificate of origin is requested

	providing information on the certificate of origin (ESS.VN.OPR.005)
	certificates of origin
(ESS.VN.BEN.001):
information on the issued certificate of origin is provided  certificates of origin
(ESS.VN.BEN.001):
information on the issued certificate of origin is absent

	receiving information on the certificate of origin (ESS.VN.TRN.002)







The scheme of the transaction «Providing information on the issued certificate of origin» (ESS.VN.TRN.001) is provided in Figure 4.


[image: C:\Users\t.abylkasymova\Pictures\8888.png]
Figure 4. Scheme of the transaction Providing information on the issued certificate of origin” (ESS.VN.TRN.001)

The scheme of the transaction «Receiving information on the certificate of origin» (ESS.VN.TRN.002) is provided in Figure 5.
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Figure 5. Scheme of the transaction «Receiving information on the certificate of origin» (ESS.VN.TRN.002)

The parameters of the transactions «Providing information on the issued certificate of origin» (ESS.VN.TRN.001) and «Receiving information on the certificate of origin» (ESS.VN.TRN.002) are listed in Subsection 9.4 of these Technical Specifications.

VI. Content and structure of information transmitted
6.1. Content of information transmitted
Description of the content of information transmitted is provided in Appendix A.

6.2. Structure of information transmitted
Description of structures of information transmitted and rules for their filling out and control is provided in a set of tables in Appendix B.
Description of the structure of transmitted information and messages in W3C language notation of XML-schemes is provided in Appendix C.
Examples of transmitted information and messages in the form of XML-documents are provided in Appendix D.
Information about web services standards is provided in Appendix F.

VII. Structure and format of messages
7.1. General requirements and applicable standards
The information transmitted as a part of the described business process, shall be XML-formatted in accordance with the Extensible Markup Language (XML) 1.0 standard (Fifth Edition) that can be found at: http://www.w3.org/TR/REC-xml.
When describing the structure and format of messages, the namespaces given in Table 12 are used, as well as the specifications provided in Table 13.

Table 12
List of XML-document namespaces

	Prefix
	Address


	soap
	http://www.w3.org/2003/05/soap-envelope

	wsa
	http://www.w3.org/2005/08/addressing

	xs

	http://www.w3.org/2001/XMLSchema




A message in SOAP format transmitted between electronic information exchange participants is made in accordance with the SOAP 1.2 specification and consists of a header block (soap:Header) and a body block (soap:Body).
The header block contains technological information required for routing and processing of a message, as well as for monitoring of electronic information exchange.

Table 13

Specifications used to describe structure and format of messages


	Short name

	Full name


	
SOAP 1.2


	SOAP Version 1.2 Part 1: Messaging Framework (Second Edition). W3C Recommendation 27 April 2007.
 http://www.w3.org/TR/soapl2-partl


	
WS-Addressing 1.0-Core

	Web Services Addressing 1.0 - Core. W3C Recommendation 
9 May2006. http://www.w3.org/TR/ws-addr-core


	
XML 1.0

	Extensible Markup Language (XML) 1.0 (Fifth Edition). W3C Recommendation 26 November 2008. http://www.w3.org/TR/2008/REC-xml-20081126
 




The body block includes the application or technological information important for the participants of electronic information exchange and shall conform with the structure of transmitted data specified in Appendix В and W3C language notation of XML-schemes specified in Appendix C.
UTF-8 encoding shall be used for generating messages and contents of their blocks. The maximum length of a message transmitted is 100 MB.
The list of business process messages transmitted within the information interaction when implementing the business process is given in Table 14.

Table 14
The list of messages transmitted

	Structure identifier
(message identifier)

	Type of information
	Purpose

	Certificate
(ESS.VN.MSG.001)

	information on the issued
certificate of origin

	contains information on the issued (annulled, recalled) certificate of origin provided by the authorized owning body

	Response
(ESS.VN.MSG.002)

	notice on the results of
processing of information


	notice on the results of processing of information on the issued (annulled, recalled) certificate of origin provided by the receiving customs authority

	Response
(ESS.VN.MSG.003)

	notification on absence of
information

	notification on results of processing of request by the authorized body-information owner, containing information about absence of requested information

	Request
(ESS.VN.MSG.004)


	request for information about the certificate of origin

	contains a request of the customs authority- information receiver for information about the certificate of origin

	Certificate (ESS.VN.MSG.005)



	information	on the 
certificate of origin provided in response to the request

	contains information on the issued (annulled, recalled) certificate of origin provided by the authorized owning body in response to the request



7.2. The structure of header blocks
The header block contains headers in accordance with WS-Addressing 1.0 – Core specification, as well as specialized headers used to organize interaction.
The header block includes the following headers:
a) wsa:To - a header containing information on the receiver;
b) wsa:From - a header containing logical address of the sender, to which the response message should be sent;
c) wsa:MessageID - a header containing message identifier;
d) wsa:RelatesTo - a header containing message reference identifier;
e) wsa:Action - a header identifying message content;
The wsa:To header is obligatory to fill out and shall include the logical address of the receiver. The logical address is used to identify the receiver in messages between the External Gateway and electronic information exchange services provided by the National Single Window of Viet Nam.
The wsa:From header is obligatory to fill out and shall include the logical address of the sender.
The list of logical addresses of participants of electronic information exchange ithin the Electronic Origin Certification and Verification System is given in Table 15.

Table 15
The list of logical addresses of participants of electronic data exchange

	Logical address of the
exchange participant
	Participant of electronic information exchange

	ESS.VN.AM
	The State Revenue Committee of the Republic of Armenia;
The Chamber of Commerce and Industry of the Republic of Armenia

	ESS.VN.BY
	The State Customs Committee of the Republic of Belarus;
The Chamber of Commerce and Industry of the Republic of Belarus

	ESS.VN.KZ

	The State Revenue Committee of the Ministry of finance of the Republic of Kazakhstan;
The National Chamber of Entrepreneurs of the Republic of Kazakhstan

	ESS.VN.KG
	The Customs Service under the Ministry of Finance of the Kyrgyz Republic;
The Chamber of Commerce and Industry of the Kyrgyz Republic

	ESS.VN.RU
	The Federal Customs Service (the Russian Federation);
The Chamber of Commerce and Industry of the Russian Federation

	ESS.VN.VN



	The Ministry of Finance (General Department of Viet Nam Customs) of the Socialist Republic of Viet Nam;
The Ministry of Industry and Trade of the Socialist Republic of Viet Nam.



The wsa:MessageID header is obligatory to fill out and is intended for unique identification of separate message instances. Values of message identifiers shall be globally unique and be UUID in accordance with RFC 4122 specification.
The wsa:Action header is intended for informing participants of the electronic information exchange on the business process procedure within which a message was sent.
The wsa:RelatesTo header is intended for message chains creation.
The wsa:RelatesTo header shall contain a value of the wsa:MessageID header of the original message. In this case, the wsa:MessageID header shall be filled with a new value.
The wsa:Action header of an applied message transmitted as part of a business process is filled out by the uniform resource identifier (URI), consisting of the following components, divided by slash-symbol
a) fixed prefix «tr://»;
b) CERTIFICATE identifier;
c) components of information on the message contents.
Components of information about the contents of the message are specified in the following order:
a) version of the interaction services;
b)  procedure code defined in Table 2 of these Technical Specifications;
c) transaction code defined in Table 11 of these Technical Specifications;
d) message code defined in Table 14 of these Technical Specifications;
Example of filling out the wsa:Action header:
tr://CERTlFICATE/0.1/ESS.VN.PRC.001/ESS.VN.TRN.001/ESS.VN.MSG.001.

VIII. Use of directories and classifiers
Special directories and classifiers are used for electronic information exchange.
Lists of directories and classifiers used within the electronic information exchange are provided in Tables 16-18.
Table 16
The list of main directories and classifiers used by all electronic information exchange participants

	Name

	Type

	Description

	

	country classifier

	the classifier
	contains the list of codes and names of countries (used in accordance with ISO 3166)
	https://www.iso.org/ob p/ui/#iso:std:iso:3166:- 1:ed-3:vl :en,fr

	language classifier
	the classifier
	contains the list of codes
and names of languages in accordance with IETF RFC 5646 and IANA
Language Subtag Registry
	https://tools.ietf.org/ht
ml/rfc5646 and https://www.iana.org/as signments/language- subtag- registry/language- subtag-registry

	classifier of cargoes, packages and packaging materials
	the classifier
	contains the list of codes and names of types of cargo, packages and packaging materials
	https://www.unece.org/ fileadmin/DAM/cefact/ recommendations/rec2 1/гес21 rev 1 ecetrd 195 e.pdf

	UN EDIFACT Code list
3031 Types of addresses
	the classifier
	contains the list of codes
and names of address
types
	https://unece.org/filead
min/DAM/trade/untdid
/d15a/tred/tred3131.ht
m

	UN EDIFACT Code list 3155 Types of communications

	the classifier
	contains the list of codes
and names of
communication types
	https://unece.org/filead
min/DAM/trade/untdid
/d 13a/tred/tred3155.ht
m




Table 17
List of directories and classifiers used by the 1Member States

	Name

	Type
	Description

	

	a Unified goods nomenclature of foreign economic activity of the Eurasian Economic Union based on the Harmonized Description and Coding System of the World Customs Organization
	the classifier
	contains the list of codes
and names of goods
	https://eec.eaeunion.org
/comission/department/
catr/ett/
https://eec.eaeunion.org
/comission/department/
catr/psn/


	units of measurement
classifier

	the classifier
	contains the list of codes, names and symbols of units of measurement
	https://portal.eaeunion.
org/sites/odata/_layouts
/15/Portal.EEC.Registr y.Ui/DirectoryForm.as px?ViewId=61f9080c- 730e-4dfb-addb- 2e6bl ld5e84b&List!d
=0e3ead06-5475-466a-
a340-
6f69c01b5687&ltemld
=283#


	classifier of transport and transportation of goods currency qualifier
	the classifier
	contains the list of types of vehicles and transportation of goods and the corresponding codes
	https://portal.eaeunion.
org/sites/odata/_layouts
/15/PortaI.EEC.Registr
y.Ui/DirectoryForm.as px?View!d=61f9080c- 730e-4dfb-addb-
2e6b11d5e84b&ListId
=0e3ead06-5475-466a-
a340-
6f69c01 b5687&Itemld
=272#


	classifier of documents used for customs declaration
	the classifier
	contains a list of codes and
names types of documents and information used for customs declaration
	https://portal.eaeunion.
org/sites/odata/Jayouts
/15/Portal.EEC.Process 11/TreeListForm.aspx? ViewId=TreeView&Lis tId=0e3ead06-5475- 466a-a340-
6f69c01 b5687&ltemld
=277





Table 18
List of directories and classifiers used 
by the Socialist Republic of Viet Nam

	Name

	Type
	Description
	

	Harmonized System (HS Code),
compatible with ASEAN Harmonized Tariff Nomenclature (AHTN)
	the classifier

	contains the list of codes and names of goods

	To be provided by the Socialist Republic of Viet Nam

	units of measurement
classifier

	the classifier

	contains the list of codes and names of units of measurement
	To be provided by the Socialist Republic of Viet Nam

	classifier of transport and transportation of goods currency qualifier

	the classifier

	contains the list of types of vehicles and transportation of goods and the corresponding codes
	To be provided by the Socialist Republic of Viet Nam


	classifier of documents used for customs declaration
	the classifier

	contains a list of codes and names types of documents used for customs declaration
	To be provided by the Socialist Republic of Viet Nam





The contents of detailed information from directories and classifiers and their structures are defined in Appendix E.
Directories and classifiers shall be updated when new versions are released.
Participants of electronic information exchange routinely exchange updated versions of directories and classifiers defined in Appendix E.
The participants of electronic information exchange shall solely track changes of versions of the directories and classifiers defined in tables 16-18 using open sources.

IX. Technical aspects and interaction parameters
9.1. General information
The procedure of information interaction during the implementation of the business processes is defined in Section V of these Technical Specifications.
When a transaction is executed, each of the sent messages shall be processed successfully, or all the application-level changes in the systems of the participants of electronic information exchange made due to processing of the transaction messages shall be cancelled.
As a part of the transactions, the following types of messages are used:
business process messages, acknowledgment signals, exception signals.
The list of business process messages is provided in Table 18 of these Technical Specifications.
A business process message is an applied message, which contains a set of applied data transmitted between the participants of electronic information exchange in accordance with the rules given in Section 5.3 of these Technical Specifications.
The acknowledgment signal is an applied message reporting on successful stage of business process message processing.
The exception signal is an applied message reporting on deviation from thebusiness process message routine processing.
Description of acknowledgment and exception signals is provided in Section 9.5 of these Technical Specifications.
In order to implement a reliable information interaction it is possible to resend a business process message, if no response or an error process message was received.
When resending the message, a new wsa:MessageID identifier shall be generated.
To ensure communication between the messages within a transaction, wsa:RelatesTo field is filled out for all the business process messages, except those initiating a transaction.
Wsa:RelatesTo field contains a wsa:MessageID identifier obtained by the participant of electronic information exchange at the previous stage of the transaction.
In order to ensure control (tracking) of duplicates (resent messages), the applied data structures shall be controlled. In this case, if the Respondent finds that the message is resent by the Initiator, the Respondent shall regenerate and send a response.
9.2. Message exchange procedure
During the execution of a transaction (for all transactions defined in Section 5.3 of these Technical Specifications), the following messaging sequence is implemented:
the initiator sends a request to the respondent and waits for confirmation of receipt of the request till the time determined in the scope of transaction parameters as a deadline for confirmation of receipt expires;
the respondent receives the request and conducts the process and structural control in accordance with the rules specified in Section 9.3 of these Technical Specifications, and sends a «Received» acknowledgment signal to the initiator;
after processing of the «Received» acknowledgment signal from the respondent, the Initiator waits for confirmation of acceptance of the information contained in the request for processing till the time determined in the scope of transaction parameters as a deadline for confirmation of processing expires;
the respondent controls the data in the request in accordance with the rules specified in Section 9.3 of these Technical Specifications, and confirms the acceptance of information received for processing by sending an «Accepted for processing» acknowledgment signal to the Initiator;
after processing the «Accepted for processing» acknowledgment signal from the respondent, the initiator waits for a response with information till the time determined in the scope of transaction parameters as a deadline for receiving a response expires;
the respondent processes the received request and sends a response to the initiator;
the initiator controls data contained in the response in accordance with the rules specified in Section 9.3 these Technical Specifications.
The order transaction given in Figure 6.




[image: C:\Users\t.abylkasymova\Pictures\3333.png]
Figure 6. The order of transaction

9.3. Procedure of message processing by receiver
Message processing is performed by the receiver receiver (the respondent in accordance with the following standard stages:
a) process control of the message;
b) structural control of the body block;
c) processing of the body block data.
The process control of a message involves checking the message structure for compliance  with the established formats avd structures of messages without regard to the applied data transmitted, a well as checking the connectivity of messages at the message header level. 
If process control of a message results in errors and checked message is not an error process message, the respondent shall send a soap:Sender error message to the initiator in accordance with the WS-Addressing 1.0 – Binding specification under the terms specified in Section 9.6 of these Technical Specifications.
The structural control of the body block involves checking its structure for compliance with the established data structures (according to XSD schema).

9.4. Parameters of transactions
Transactions shall be carried out in accordance with the given transaction parameters.
The parameter «Time to confirm receipt» sets the maximum time period between sending a business process message by the initiator and the time of receipt of the acknowledgment signal «Received».
The initiator of the business process message shall resend the message if the respondent has not confirmed the receipt within an agreed period of time. The number of retries is set using the parameter «Number of retries».
The parameter «Time to confirm acceptance for processing» sets the maximum period of time between sending a business process message by the initiator and the time of receipt of the acknowledgment signal «Accepted for processing».
The initiator of request shall resend the message if the respondent has not confirmed the receipt within the agreed period of time. The number of retries is set using the parameter «Number of retries».
The parameter «Time to respond» sets the maximum period of time between sending a business process message (request) by the initiator and the time of receipt of the respondent»s response with the information on the results of processing of the request (response).
The initiator shall resend the request, if no response has been received from the respondent within the agreed period of time. The number of retries is set using the parameter «Number of retries».
Control over the observance of procedural deadlines set by the parameters «Time to confirm receipt», «Time to confirm acceptance for processing» and «Time to respond» is the initiator»s responsibility. The Respondent bears no responsibility for control of these parameters.
The parameter «Number of retries» sets the maximum number of retries of business process messages.
The situation when all the retries of sending a business process message have been exhausted and the required messages have not been received by the initiator is emergency. The procedure for actions performed by the parties in emergency situations is specified in Section XI of these Technical Specifications.

9.4.1.Parameters of the transaction «Providing information on the issued certificate of origin»
Parameters of the transaction «Providing information on the issued certificate of origin» (ESS.VN.TRN.001) are given in Table 19.

Table 19
Description of the transaction «Providing information on the issued certificate of origin» (ESS.VN.TRN.001)

	No.
	Parameter
	Description

	1
	Designation

	ESS.VN.TRN.001

	2
	Name of transaction

	providing information on the issued certificate of origin

	3
	Initiator

	authorized body-information owner

	4
	Initiation operation

	transferring information on the issued certificate of origin
(ESS.VN.OPR.001 )

	5
	Respondent

	customs authority-information receiver


	6
	Receiving operation
	receiving and processing of information on the issued
certificate of origin (ESS.VN.OPR.002)

	7
	Result of transaction

	certificates of origin (ESS.VN.BEN.001): information on
the issued certificate of origin is received


	8
	Parameters of transaction:

	

	
	time to confirm receipt
	5 min

	
	time to confirm
acceptance for

	20 min

	
	processing

	

	
	time to wait for response
	20 min


	
	number of retries
	3

	9
	Messages of transaction:

	

	
	initiation message
	information on the issued certificate of origin
(ESS.VN.MSG.001)


	
	response message

	notice of the results of processing of information
(ESS.VN.MSG.002





9.4.2. Parameters of the transaction «Receiving information on the certificate of origin»
Parameters of the transaction «Receiving infonnation on the certificate of origin» (ESS.VN.TRN.002) are given in Table 20.
Table 20
Description of the transaction «Receiving information on the certificate of origin» (ESS.VN.TRN.002)

	No.
	Parameter
	Description

	1
	Designation
	ESS.VN.TRN.002

	2
	Name of transaction
	receiving information about the certificate of origin

	3
	Initiator
	customs authority-information receiver

	4
	Initiation operation

	requesting for information on the certificate of origin (ESS.VN.OPR.004)

	5
	Respondent
	authorized body-information owner

	6
	Receiving operation
	providing information	on	the certificates	of origin (ESS.VN.OPR.005)

	7
	Result of transaction
	certificates of origin (ESS.VN. BEN.001): information on the certificate of origin is absent
certificates of origin (ESS.VN.BEN.001): information on the issued certificate of origin is provided

	8
	Parameters of transaction:

	

	
	     time to confirm receipt
	5 min

	
	time to confirm  
acceptance for 
processing
	5 min

	
	time to wait for response
	10 min


	
	     number of retries
	3

	9
	Messages of transaction:

	

	
	initiation message
	request for information about the certificate of origin
(ESS.VN.MSG.004)



	
	response message

	providing information on the certificate of origin
(ESS.VN.MSG.005);
notice on absence of information (ESS.VN.MSG.003)





9.5. Acknowledgment signals and exception signals
The namespaces used for description of the structure and the requisite composition of acknowledgment signals and exception signals are given in Table 21.
Table 21
Namespaces
	Prefix
	Address

	xs
	http://www.w3.org/2001/XMLSchema

	sgn
	urn: certificate:signal:v 1.0



The base data types used for description of the structure and the requisite
composition of acknowledgment signals and exception signals are given in Table 22.

Table  22
Base data types

	Name
	Description

	sgn:EDocIdType
	the document identifier, which is a UUID in accordance with standard
ISO/IEC 9834-8:2005.
String of symbols with framework [0-9a-fA-F]{8}-[0-9a-fA-F]{4}-[0-9a-fA-F]{4}-[0-9a-fA-F]{4}-[0-9a-fA-F]{12}


	sgn:DateTimeType
	the Gregorian calendar date and time in the format of ISO 8601 “Data elements and interchange formats – Information interchange –Representation of dates and types”

	sgn:ErrorCodeType
	designation of the Control Error. String consists of 1 to 255 symbols


	sgmStringType
	textual arbitrary information. A string is of arbitrary length







9.5.1. The acknowledgment signal «Received»

The respondent will send the acknowledgment signal «Received» at the moment when the step of the structural block content control is made.
P.MSG.RCV message code for the acknowledgment signal «Received» will be used when the wsa:Action header, identifying the contents of the business process message, is formed. Other components of the data on message content are specified in accordance with the rules for forming the wsa:Action header for applied messages as described in Section 7.2.
The structure and requisite composition of the acknowledgment signal
«Received» are given in Table 23.
Table 23
The structure and requisite composition of the acknowledgment signal «Received»
	Element

	Data type
	Description

	Mult


	sgmDcliveryReceipt
	sgn:DeliveryReceiptType
	wrapping	element of the acknowledgment signal «Received»
	

	
	sgn:Signalld
	sgn:EDocIdType
	signal identifier
	1

	
	sgn:DateTime	
	sgn:DateTimeType
	date and time of the acknowledgment signal fomring «Received»
	1




9.5.2. The acknowledgment signal «Accepted for processing»
The acknowledgment signal «Accepted for processing» is sent by a respondent before processing of the body block data.
P. MSG.PRS message code for the acknowledgment signal «Accepted for processing»will be used when the wsa:Action header, identifying the contents of the business process message, is formed.
Other components of the data on message content are specified in accordance with the rules of forming of the wsa:Action header for applied messages as described in Section 7.2 of these Technical Specifications.
The structure and requisite composition of the acknowledgment signal «Accepted for processing» are given in Table 24.


Table 24
The structure and requisite composition of the acknowledgment signal «Accepted for processing»
	Element

	Data type
	Description
	Mult

	sgn:ProcessingReceip
t

	sgn:Processing
ReceiptType
	wrapping element of the acknowledgment signal «Accepted for processing»
	

	
	sgnrSignalld
	sgn:EDocIdType
	signal identifier
	1

	
	sgn.»DateTime

	sgn:DateTimeType
	date and time of the acknowledgment signal forming «Accepted for processing»
	1



9.5.3. The exception signal «Error»
The situation, when the respondent sends the exception signal «Error» to the initiator, occurs in the following cases:
a) the respondent has accepted the business process message, which was not expected to be received within a transaction execution;
b) the respondent has found errors during the structural control of the body block or format-logic control of the body block;
c) an unrecoverable error, making it impossible to perform applied data processing, occurred on the applied data processing step.
The situation, when the respondent has received the business process message, which was not expected to be received within a transaction execution, occurs in the following cases:
the message received is a business process message or an acknowledgment signal, and thus it does not apply to transactions executed by the respondent;
the respondent is not authorized to process the message received (if they do not participate in information interaction, procedure or transaction).
In these cases, the value (code) «Common:UnexpectedMessage» is assigned to the designation of Control Error (field sgn:Code) of the exception signal «Error».
If the respondent finds an error during the structural control of the body block, the value (code) «Common:Data Error»  is assigned to the designation of Control Error (box sgn:Code) of the exception signal «Error».
If the respondent finds an error during the format-logical control of the business process message, the value of rule code is assigned to the designation of Control Error (sgn:Code field) of the exception signal «Error», within checking of which an error occurred according to Table 29.
If there is a situation, when an unrecoverable error occurred on the step of body block data processing, making it impossible to perform data processing, the value (code) «Common:FatalError» is assigned to the designation of Control Error (field sgn:Code) of the exception signal “Error”.
List of unrecoverable errors is determined by the participant of electronic information exchange independently.
P.MSG.ERR message code for the exception signal «Error» will be used when the wsa:Action header, identifying the contents of the business process message, is formed. Other components of the data on message content are specified in accordance with the rules of forming of the header wsa:Action for applied messages.
The structure and requisite composition of the exception signal «Error»are given in Table 25.
  Table 25
The structure and requisite compositon of the exception signal «Error»
	Element

	Data type
	Description

	Mult

	sgn:ValidationError
	sgn:ValidationError Type

	wrapping element of the exception signal «Error»
	

	
	sgn:SignalId
	sgn:EDocIdType
	identifier of the exception signal «Error»
	1

	
	sgn.DateTime
	sgn:DateTimeType
	date and time of the exception signal forming «Error»
	1

	
	sgn:Error
	sgn:ErrorType
	wrapping element
	1 . *

	
	
	sgn:Code
	sgn:ErrorCodeType

	error designation
	1

	
	
	sgn:Description
	sgn:StringType
	error text value
	1

	
	
	sgn:Details

	sgn:StringType
	error detailed data
	0.1

	
	
	sgn:EDocId
	sgn:EDoc ld Type
	document identifier, in which the error occurs. It is completed if the error is related to a certain document and the document identifier was extracted
	0.1

	
	
	sgn:Reference
	sgmStringType
	a string of symbols that 
allows to uniquely locate 
the item that caused the error
	0.1



To participate in the information interaction, the participants of electronic information exchange shall implement the services enforcing Business Process Procedures on their side.
Description of services in WSDL-format is given in Appendix F.

9.6. Error process message
If an error occurs at the step of the process control of a message, an error process message shall be formed. Error process message body block shall contain elements specified in Table 26.
Table 26
Composition of the process message body block
	Element


	Data type
	Description
	Mult

	soap:Fault
	soap:Fault
	block wrapping element


	

	
	soapr:Code
	soap:faultcode
	wrapping element
	1

	
	
	soap:Value
	soap:faultcodeEnum
	error class
	1

	
	
	soap:Subcode
	soap:subcode
	error code wrapping element
	1

	
	
	
	soap:Value
	xs:OName
	error code
	1

	
	soap:Reason
	soap:faultreason
	wrapping element of the error text	
description

	1

	
	
	soap:Text


	soap:reasontext
	block of the error text description
	1 ..*

	
	
	
	@xml:lang
	–
	language identifier
	1

	
	soap:Detail

	soap:detail

	error details
	0.1



The soap:Code/soap:Value element shall be completed in accordance with SOAP 1.2 specification.
The soap:Code/soap:Subcode/soap:Value element shall contain an error code. 
The list of standard error codes and rules on the use of codes from WS- ddressing 1.0 - Binding specification are provided in Table 27.
Table 27
Typical errors codes
	Error
class

	Error code
	Description and application features

	soap:Sender
	wsa:dnvalidAddressingHea
der
	used in accordance with the rules defined by WS- Addressing 1 .О-Binding specification with the following restrictions: Subsubcode values are not used, wsa:DuplicateMessageID error type is not generated and is not sent

	soap:Sender
	wsa:MessageAddressingHe
aderRequired

	used according to the rules, defined by WS-Addressing 1.0-Binding specification 

	soap:Sender
	wsa:DestinationUnreachable
	used according to the rules, defined by WS-Addressing 1.0-Binding specification

	soap:Sender
	wsa:ActionNotSupported
	used according to the rules, defined by WS-Addressing 1.0-Binding specification


	soap:Sender
	intdnvalidHeader
	one or more specific headers are missing

	soap: Receiver
	wsa:EndpointUnavailable
	used according to the rules, defined by WS-
Addressing 1.0-Binding specification with the following restrictions: the element wsa:RetryAfter shall not be used while implementation of the electronic information
exchange

	soap: Receiver
	int:IntemalError
	an unexpected error occurred while processing the message

	soap:Sender

	int:DataError
	received applied data have an incorrect structure



The soap:Text element shall contain the error text description.
Each soap:Text element shall contain the xmhlang language identifier, formed in accordance with XML 1.0 specification.
If there is a set of soap:Text elements in the error process message, each of these elements shall contain the xmhlang language identifier, that differs from the IDs of other soap:Text elements.
The error process message shall contain at least one soap:Text element, the contents of which is presented in English, and the xmldang language identifier shall contain «en» value. 
The soap:Detail optional element shall include information detailing the error.

9.7. Services technical implementation

Electronic information exchange between the External Gateway and information interaction services provided by National Single Window of Viet Nam is performed using SOAP services.
The SOAP service shall be implemented on each side, both the External Gateway and Viet Nam side.
To implement electronic information exchange within the EOCVS defined in these Technical Specifications, EECVNCERTIFICATION service shall be used.
The list of EECVNCERTIFICATION service methods is given in Table 28.
Table 28
List of EECVNCERTIFICATION service methods

	No.

	Method
	Description

	1
	sendCertificateDetails
	providing information on the issued certificate of origin

	2
	sendRequestCertificateDetails
	receiving information about the certificate of origin

	3
	sendResultCertificateDetails


	receiving results of processing containing information on the certificate of origin

	4
	sendSignal
	receiving of signals on the current processing status

	5
	sendResult
	receiving of the processing result




9.7.1. The method «sendCertificateDetails»

Purpose: implementation of the operation “Receiving and processing of information on the issued certificate of origin” (ESS.VN.OPR.002)
Business process procedure: ESS.VN.PRC.001
SOAP method: sendCertificateDetails
Description: providing information on the issued certificate of origin (carried out by calling the sendCertificateDetails method by the respondent (receiver) of the message «Information on the issued certificate of origin» (ESS.VN.MSG.001)).
Input parameters: ESS.VN.MSG.001 (Certificate)
Output parameters: no data
Description of the operation algorithm:
Message processing steps within the execution of the service shall comply with the rules specified in Section 9.3 of these Technical Specifications:
1. Process control of the message;
2. Structural control of the body block;
3. Processing of the data block.
For the services, being implemented on Viet Nam side, all the message processing stages shall be executed.
For the services implemented on the External Gateway, steps 1 and 2 shall be executed. Processing step 3 is implemented and executed within Information Systems of the receiving customs authorities of the Member States.
Structural control of the body block involves the check of the message structure «Information on the issued certificate of origin» (ESS VN.MSG.001) for compliance with the structure «Information on the certificate of origin» (Certificate) provided in Appendices В and C of these Technical Specifications.
If the results of message process control and body block structural control are successful, the acknowledgment signal «Received» shall be generated and sent. The acknowledgement signal «Received» is transmitted by calling the method «Receiving of signals on the current processing status» (sendSignal) on the side of the original message sender.
If process control of the message resulted in errors, the receiver shall send an error process message of the soap:Sender class to the sender. A detailed description of the error process message is provided in Section 9.6 of these Technical Specifications.
Before processing of the body block data, the acknowledgment signal «Accepted for processing» shall be generated and sent. The acknowledgement signal «Accepted for processing» is transmitted by calling the method «Receiving of signals on the current processing status» (sendSignal) on the side of the original message sender.
Requirements for the method of message body block data processing and requirements for the storage of message processing results are defined by information interaction participants.
If the body block data is processed successfully, the message  «Notice on the results of processing of information» (ESS.VN.MSG.002) containing results of processing of information on the certificate of origin shall be prepared and sent. The message is transmitted using the method «Receiving of processing result» (sendResult) on the side of the original message sender.
If an error occurred during the body block data processing, the exception signal «Error» shall be prepared and sent in accordance with the rules from Section 9.5.3 of these Technical Specifications.
The list of potential errors within the implementation of the transaction «Providing information on the issued certificate of origin» (ESS.VN.TRN.001) is given in Table 29.
Table 29

	Error code
	Error description
	Description of checking within body block processing

	


1
	Duplication error. Registration number of the certificate is found among previously transmitted certificates.

	The CancellationDateTime («Date of certificate annulment») requisite is not filled within previously provided information on the issued certificate, and the «Certificate registration number» ID requisite value is found within previously transferred certificates



The exception signal «Error» is transmitted by calling the method «Receiving of signals on the current processing status» (sendSignal) on the side of the original message sender.

9.7.2. The method «sendRequestCertificateDetails»

Purpose: implementation of the operation “Providing information on the certificate of origin» (ESS.VN.OPR.005)
Business process procedure: ESS.VN.PRC.002
SOAP method: sendRequestCertificateDetails
Description: receiving information on the certificate of origin (carried out by calling the sendRequestCertificateDetails method on the receiver side of the message «Request for information on the certificate of origin» (ESS.VN.MSG.004)).
Input parameters: ESS.VN.MSG.004 (Request)
Output parameters: no data
Description of the operation algorithm:
Message processing steps within the execution of the service shall comply with the rules specified in Section 9.3 of these Technical Specifications:
Process control of the message;
Structural control of the body block;
Processing of the data block.
For the services, being implemented on Viet Nam side, all the message processing stages shall be executed.
For the services implemented on the External Gateway, steps 1 and 2 shall be executed. Processing stage 3 is implemented and executed in information systems of the authorized body-information owner of Member States.
Structural control of the body block involves the check of the message structure «Request for information on the certificate of origin» (ESS.VN.MSG.004) for compliance with the structure «Request for information on certificates of origin» (Request) provided in Appendices В and C of these Technical Specifications.
If the results of message process control and body block structural control are successful, the acknowledgment signal «Received» shall be generated and sent. The acknowledgement signal «Received» is transmitted by calling the method «Receiving of signals on the current processing status» (sendSignal) on the side of the original message sender.
If process control of the message resulted in errors, the receiver shall send an error process message of the soap:Sender class to the sender. A detailed description of the error process message is provided in Section 9.6 of these Technical Specifications.
If the information that satisfies the request was found, the message «Providing information on the certificate of origin» (ESS.VN.MSG.005) containing the information found shall be generated and sent. The message is transmitted using the method «Receiving of processing results containing information on the certificate of origin» (sendResultCertificateDetails) on the side of the original message sender.
If the information that satisfies the request was not found, the message «Notice on absence of information» (ESS.VN.MSG.003) shall be generated and sent. The message is transmitted using the method «Receiving of processing result» (sendResult) on the side of the original message sender.
If an error occurred during the body block data processing, the exception signal «Error» shall be prepared and sent in accordance with the rules from Section 9.5.3 of these Technical Specifications.

9.7.3. The method «sendResultCertificateDetails»
Purpose: implementation of the operation «Receiving and processing of information on the issued certificate of origin» (ESS.VN.OPR.006);
Business process procedure: ESS.VN.PRC.002; SOAP method: sendResultCertificateDetails
Description: receiving the results of processing containing information on the certificate of origin (carried out by calling the sendResultCertificateDetails method on the receiver side of the message «Information on the certificate of origin provided in response to the request» (ESS.VN.MSG.005)).
Input parameters: ESS.VN.MSG.005 (Certificate)
Output parameters: no data
Description of the operation algorithm:
Message processing steps within the execution of the service shall comply with the rules specified in Section 9.3 of these Technical Specifications:
1. Process control of the message;
2. Structural control of the body block;
3. Processing of the data block.
For the services, being implemented on Viet Nam side, all the message processing stages shall be executed.
For the services implemented on the External Gateway, steps 1 and 2 shall be executed. Processing step 3 is implemented and executed within Information Systems of the receiving customs authorities of the Member States.
Structural control of the body block involves the check of the message structure «Information on the issued certificate of origin provided in response to the request» (ESS.VN.MSG.005) for compliance with the structure «Information on the certificate of origin» (Certificate) provided in Appendices В and C of these Technical Specifications.
If process control of the message resulted in errors, the receiver shall send an error process message of the soap:Sender class to the sender. A detailed description of the error process message is provided in Section 9.6 of these Technical Specifications.
Requirements for the method of message body block data processing and requirements for the storage of message processing results are defined by information interaction participants.
If an error occurred during the body block data processing, the exception signal «Error» shall be prepared and sent in accordance with the rules from Section 9.5.3 of these Technical Specifications. 
The exception signal «Error» is transmitted by calling the method «Receiving of signals on the current processing status» (sendSignal) on the side of the original message sender. 

9.7.4. The method «sendSignal» 
Purpose: Implementation of receiving and processing of acknowledgment signals and exception signals.
Business process procedure:
ESS.VN.PRC.001;
ESS.VN.PRC.002;
SOAP method: sendSignal
Description: Receiving of signals on the current processing status
Input parameters:
P.MSG.ERR P.MSG.PRS P.MSG.RCV
Output parameters: no data
Description of the operation algorithm:
The procedure is defined by the signal type and transaction during which the signal was received (see Section 5.3 of these Technical Specifications).

9.7.5. The method «sendResult»
Purpose: Implementation of the following operations:
«Receiving and processing of the notice on the results of processing of information on the issued certificate of origin» (ESS.VN.OPR.003);
«Receiving and processing of information on the certificate of origin» (ESS.VN.OPR.006);
Business process procedure:
ESS.VN.PRC.001; 
ESS.VN.PRC.002;
SOAP method: sendResult
Description: Receiving of data processing result
Input parameters:
ESS.VN.MSG.002;
ESS.VN.MSG.003;
Output parameters: no data
Description of the operation algorithm:
The procedure is defined by the message code and transaction, during which the signal was received (see Section 5.3 of these Technical Specifications).


X. Information protection
The information transmitted within the business process is the information of restricted access (confidential information), the access of third parties to this information is limited, and its uncontrolled distribution is not allowed.
The Member States, the Socialist Republic of Viet Nam and the Commission shall protect information in its transferring, receiving and processing within their area of responsibility.
When information is transferred within the information space of the Member State, it is protected in accordance with the legislation and technical requirements for ensuring information protection in force on the territory of the Member State concerned.
When transmitting information within the information space of Viet Nam, the protection is ensured in accordance with the legislation and the technical requirements for information protection in force on the territory of Viet Nam.
The Commission and the General Department of Viet Nam Customs shall protect information transmitted between the IIS and the National Single Window of Viet Nam.
When transmitting information using IIS functions of protection of information from unauthorized access, information security and permanence upon unauthorized or accidental impacts is provided by means of IIS.
When transmitting and receiving information through communication channels between the External Gateway and the National Single Window of Viet Nam, the information shall be protected by means of virtual private network (VPN) using hardware-software and/or software solutions. The authentication of the interacting parties and the encryption of the transmitted data shall be organized using the IPSec (RFC 2401-2412) and IPlir (PI 323565.1.034-2020) protocols.
To implement cooperation with the services two cryptographic data channels shall be used:
channel for transferring data from Viet Nam to the Commission built on the Pulse Secure Gateway VPN gateway and controlled by Viet Nam;
channel for transferring data from the Commission to Viet Nam built on the VipNet Coordinator HW VPN gateway and controlled by the Commission.
Cryptographic keys for VPN channel organization are issued and withdrawn by:
from the side of the Union - by the verification center of the Commission;
from the side of Viet Nam - by the verification center of the National Single Window of Viet Nam.
To ensure the decryption of traffic and its redirection to the service, the objects of Pulse Secure Ipsec VPN Endpoint and VipNet Client Endpoint shall be used. These objects are dedicated workstations with installed VPN gateway software client.
To ensure the flotation of data through encrypted channels, asymmetric routing shall be used.
To ensure the transmission of data from the National Single Window of Viet Nam to the IIS and from the IIS to the National Single Window of Viet Nam, source and destination IP-addresses shall be defined at the electronic information exchange implementation stage.
The applicable parameters of VPN data channels are given in Table 30.

Table 30
	No
	Parameter
	IPsec
	IPlir


	
	Mode
	Tunnelling
	tunnelling


	
	Authentication
technique
	Pre-shared	key	PSK)
and public	-address
	keys and identifiers of nodes	the ViPNet network


	
	Authentication
encryption algorithm
	ESP hmac-shal-96
	GOST 28147-89	(key
length: 256 bits)

	
	Data encryption
algorithm
	3des-cbc
	GOST 28147-89	(key
length: 256 bits)

	
	IKE encryption
algorithm
	Diffie-Hellman Group 2,
3des-cbc
	
––

	
	SA lifetime
	86 400   seconds	(24
hours)
	
––

	
	SA traffic volume
	…...
	––



The information security solutions defined by these Technical Specifications shall be synchronized with the information security solutions implemented for exchange of customs information between the customs authorities of the Member States and Viet Nam and are determined by these customs authorities.


XI. Emergency procedures
The emergency situations (the situations when data cannot be processed correctly) can arise during information interaction within the Business Process Procedures. Emergency situations appear due to technical faults timeout Control Error structure and in other cases.
Receiving any error process messages when performing Business Process Procedures is an emergency situation.
In order to resolve emergency situations, the Parties and the Commission shall provide each other with the information on the persons responsible for providing technical support during the electronic information exchange, their contact details and working hours (providing for timezone differences) If an emergency situation is not caused by the availability jf specific resources, the recipient of exception signal «Error» and/or error process message, (hereinafter referred to as «the Error notice») shall review the message, in regard to which the error notification was received. For compliance with the description of formats and structures of electronic documents, information and  requirements for the message control specified in these Technical Specifications, particularly in Appendices B and  C. If the non-compliance with specified requirements is detected, the recipient shall take all necessary measures to eliminate the error and send the message again. If non-compliances are not detected, the error notice recipient shall send the message containing information on the emergency situation and the inspection results to the IIS technical support.
The IIS technical support shall review the description of the emergency situation considering the information on the results of inspection carried out by the error notification recipient, prepare guidelines for ist elimination, and carry out and/or coordinate works on the elimination in cooperation with the recipient and the sender of the error notice. 
If an emergency situation is caused by the unavailability of certain resources, the recipient shall inform the IIS technical support on the emergency situation. If necessary, the IIS technical support shall reguest additional information from the error notice sender, review the emergency situation, prepare guidelines for ist elimination, and carry out and/or coordinate works on the elimination in cooperation with the recipient and the sender of the error notice.
The authorized bodies and central customs authorities the Member States, Viet Nam and the Commission shall inform each other about maintenance works on on their information systems, while these information sistems are unable to send and receive messages, not later than 24 hours before these works start.
General recommendations for resolving emergency situations are given in Table 31.
                
Table 31 
Actions in emergency situation

	Description of emergency
situation
	Causes of emergency situation
	Description of actions in
emergency situation

	1
	2
	3

	the transaction Initiator did not receive a response message after the agreed number of retries
	technical failures in the transportation system or system software error
	send a request to the support service of the integrated information system

	the transaction Initiator
received an error message
 

	directories and classifiers are not synchronized or XML- schemas of electronic documents (information) are not updated
	the transaction initiator needs to check the structure of sent messages, synchronize directories and classifiers.
If non-compliances were not
found, the transaction Initiator sends the message describing the emergency situation to the technical support of the integrated information system

	an error occurred while processing the response message from the respondent within the Initiator»s information system
	error in checking and processing of the message content block on the side of the transaction Initiator
	the transaction Initiator shall check the content block for the correctness of the transmitted information and send a message describing the emergency situation to the technical support of the transaction Respondent



XII. Applicable standards

The list of international and industrial standards used in the electronic information exchange implementation and these Technical Specifications development is given in Table 32.
Table 32 
The list of applicable standards
	Classifier name
	Reference

	1
	2

	Classifier of transport means categories UN/Recommendation 19
	http://www. nece org/fileadmin/DAМ/cefact/re commendations/rec19/rec19–01cf19e.pdf

	Codes for types of cargo, packages and packaging
materials EDIFACT codes (7065) = UN/ECE Recommendation 21 Annex VI

	https://www. unece.org/fileadinin/DAM/cefact/r ecommendations/rec21/rec21revl ecetrd     l95e.pdf

	Country classifier EDIFACT codes (3207)= ISO  3166-2
	https://www.iso.org/ obp/ui/#iso:std:iso:3166:- 1:ed-3:vl :en,fr

	ISO 8601:2004 international standard. Representation of date and time
	https://www.iso.0rg/obp/ui/#iso:std:iso: 8 601:ed-3:vl:en

	Harmonized Commodity Description and Coding
System
	http://www.wcoomd org/en/topics/nomenclature
/instrument-and-tools/hs-nomenclature-2017-
edition/hs-nomenclature-2017-edition aspx


	ISO/IEC 9834-8:2014. Information technologu/
Procedures for the operation of object identifier registration authoritiers. Part 8: Generation of universally unigue identifiers (UUIDs)and their use in object identifiers
	https://www.iso.org/obp/ui/#iso:std:iso-iec:9834:-8:ed-3:vl:en

	UN/EDIFACT Code Lists 1001, 3035, 3131, 3155, 3207, 3229, 7065, 8053
	https://unece.0rg/fileadmin/DAM/trade/edifact/code/1001cl.htm
https://unece.Org/fileadmin/DAM/trade/untdid/d
97b/uncl/unc 13035 htm
https://unece 0rg f leadmin/DAM/trade/untdid/d
15a/tred/tred3131 htm
https://unece 0rg/f leadmin/DAM/trade/untdid/d 13a/tred/tred3155.htm https://unece.0rg/fileadmin/DAM/trade/untdid/d 14a/tred/tred3207.htm
https: /unece.Org/fileadmin/DAM/trade/edifact/c
ode/3229cl.htm
https://unece.0rg/fileadmin/DAM/trade/untdid/d
14a/tred/tred7065.htm
https://unece.0rg/fileadmin/DAM/trade/edifact/c
ode/8053cl.htm


	Extensible Markup Language (XML) 1.0 (Fifth
Edition). W3C Recommendation
	https://www w3 org/TR/2008/REC-xml-
20081126/


	ISO/IEC 40210:2011 Information technology. W3C SOAP — Version 1.2. Part 1, Part 2 and others

	https://www.iso.Org/ru/ics/35.080/x/

	ISO/IEC 19505-1-2012 Information technology. Object Management Group Unified Modeling Language (OMG UML). Part 1 : Infrastructure ISO/IEC 19505-2-2012 Information technology. Object Management Group Unified Modeling Language (OMG UML). Part 2: Superstructure

	https://www.omg.org/spec/UML/ https://www.omg.Org/spec/UML/2.5. 1 /PDF


	RFC 2401-2412
	https://www.ietf.org/rfc/ 




XIII. Implementation order
To implement the electronic information exchange, the Parties shall:
appoint persons on the part of the Participants of electronic information exchange, as well as on the part of the Commission responsible for ensuring the electronic information exchange, and perform mutual exchange of information about persons mentioned above;
synchronize directories and classifiers specified in Appendix E hereto between the Parties;
synchronize information from national directories and classifiers used for the formation of electronic messages;
modify the software of authorized bodies and central customs authorities of the Member States and Viet Nam in terms of formation and maintenance of information resources containing information on certificates of origin;
develop software components that implement the electronic information exchange;
provide secure communication channels between the External gateway and the National Single Window of Viet Nam;
perform an internal, integrated and inter-state testing; modify the software based on the test results.


Appendix A. Scope of information to be exchanged within implementation of  electronic information exchange

Table A 1
Data list from a certificate of origin

	Name of data

	Description

	Mult.


	1.Designation of the form of the certificate

	the «EAV» code of the certificate is specified
	1

	2.Designation of special marks

	the code designating the following is specified:
ORG - the issued certificate of origin is the original;
DBL - the issued certificate of origin is the duplicate of
the certificate of origin;
CHG - the certificate of origin is issued in substitution of
the original certificate of origin;
	1

	3.Data on the certificate
	data according to the list provided in Table A2 are
specified
	1

	4.Data on the country
which issued the certificate
	the code and the name of the country in which the
certificate of origin was issued is specified
	1

	5.Data on the ountry for which the certificate is issued
	the code and the name of the country for which the issued
certificate of origin is intended is specified
	1

	6.Date of annulment of the certificate

	if necessary the date of annulment (recall) of the certificateis specified
	0…1

	7.Date of modification of the certificate

	if necessary the date of modification of the certificate of
origin according to article 4.21 of FTA is specified

	0…1

	8.Code designation of the certificate category


	if necessary, the R.TR code is specified designating that
the certificate of origin was issued afterwards.

	0…1

	9.Data on earlier issued certificate

	the registration number and the date of the certificate
(issue) of earlier issued certificate of origin (according to Table A 2) are specified if the certificate of origin is duplicate or issued in substitution of the original certificate (data at number 2 are «DBL» or «CHG»).
	0…*

	10.Data on the country of origin
	the code and the name of the country of origin of goods
(the Member State of the Eurasian Economic Union or
the Viet Nam) is specified
	1

	11.Data on the authorized body
	the code of the authorized body which issued the certificate of origin including the name of authorized body is specified
	1

	12.Data of the certificate verification
	data on the place of the certificate verification are
specified
	1

	13.Information about the applicant

	data on the place and date of announcement of data and
a Iso the information about the applicant are specified
	1

	14.Data on consignment
	contain data according to the list provided in Table A3 of this Appendix
	1

	15.Date and time of recording of data
	date and time of recording of data of the certificate of
origin are specified
	1



Table A 2
Document data list
	Name of data
	Description
	Mult.

	1. Certificate identifier
	the registration number of the certificate of origin is
specified
	1

	2.Unique identification
number of the certificate
	the unique identification number of the certificate is
specified
	0…1

	3.Date of the certificate
verification (issue)
	date of the certificate verification ( issue) is specified
	1

	4.Expiration date of the
certificate
	expiration date of the certificate is specified
	1


     Table A3
Consignment data list 
	Name of data
	
	Mult.

	1 . Information about the
exporter
	information about the exporter of goods, including the name of the exporter, and the address including the country code of the exporter are specified
	

	2.Information about the
importer
	information about the importer of goods, including the name of the importer and the address including the country code are specified
	

	3.Information about the receiver (consignee) of goods
	information (if it is known) about the consignee of goods, including name of a consignee and the address including the country code is specified
	

	4.Data on a route of
transportation of goods
	data on a route of transportation of goods are specified

	

	5.Data on goods
	data according to the list provided in Table A4 of this
Appendix are specified
	



Table A4
Goods data list
	Name of data
	Description
	Mult.

	1.Sequence number
	sequence number of goods
	1

	2.Data on packaging of
goods
	data on a code of a type of packaging of goods and their name and also on the number of packagings of each type are specified
	1. .*

	3.A commodity code
according to HS
	the commodity code according to the harmonized
system at the level of 6 signs is specified
	1

	4.Description of goods
	the detailed description of goods is specified, if applicable ,the name of model and trademark allowing to identify goods

	1

	Additional marks
	the additional marks on goods provided by FTA are
specified
	

	Data on criteria of goods origin
	the code of designation of origin criterion according to the list is specified:
 
	

	Gross weight
	
	

	
	
	


Table A5
Invoice data list
	Name of data
	Description
	Mult

	1.Invoice information 
	the document type code, number and document date are specified
	1

	2.Additional features:
	if the invoice is issued in the Third Country and provided for delivery to the importing country, a of TCI is given and:
	

	2.1
	number and date of invoice, as well as the name and the country of the company which issued such invoice;
	0…1

	2.2
	information that the invoice will be issued later, as well as the trade name and the address of aphysical person or a legal entity which will issue this invoice in the Third Country;
	0…1

	2.3
	number and date of invoice of the exporter (issued in the Union/Viet Nam)
	0…1






Appendix В. Structure of information transmitted
Table В1
Imported namespaces
	№
	Namespace identifier
	Prefix

	1
	2
	3

	1
	urn:wco:datamodel:WCO:DS:l
	ds

	2
	urn:un:unece:uncefact:data:standard:QualifiedDataType:5
	qdt

	3
	http://www.w3.org/2001/XMLSchema
	xsd

	4
	urn:un:unece:uncefact:codelist:standard:UNECE:ScheduleTaskRelationshipType:D08A

	clm69673


	5
	urn:un:unece:uncefact:codelist:standard:UNECE:PaymentMeansCode:D08A
	clm64461

	6
	urn:un:unece:uncefact:codelist:standard:UNECE:ReportingThresholdTriggerType:D08A
	clm69667

	7
	urn:un:unece:uncefact:codelist:standard:UNECE:ScheduleTaskType:D08A

	clm69675

	8
	urn:un:unece:uncefact:codelist:standard:UNECE:PaymentMethodCode:D08A

	clm64439

	9
	urn:un:unece:uncefact:codelist:standard:UNECE:ResourceCostCategory:D08A


	clm69669

	10
	urn:un:unece:uncefact:identifierlist:standard:UNECE:PaymentTermsDescriptionIdentifier:D08A
	ids64277

	11
	urn:un:unece:uncefact:codelist:standard:LnSIECE:TransportModeCode:2
	clm6Recommendation19


	12
	urn:un:unece:uncefact:codelist:standard:UNECE:PriceTypeCode:D08A

	clm65375

	13
	um:un:unece:uncefact:codelist:standard:UNECE:ProjectTypeCode:D08A

	clm69665

	14
	urn:un:unece:uncefact:codelist:standard:UNECE:SecurityClassificationType:D08A

	clm69677

	15
	urn:un:unece:uncefact:codelist:standard:UNECE:ResourcePlanMeasureType:D08A

	clm69671

	16
	urn:un:unece:uncefact:codelist:standard:UNECE:PaymentGuaranteeMeansCode:D08A

	clm64431


	17
	urn:un:unece:uncefact:codelist:standard:UNECE:Transport Means Type Code:2007
	clm6 Recommendation28

	18
	urn:un:unece:uncefact:codelist:standard:UNECE:Acknowledgement:D08A
	clm61225 Acknowledgement

	19
	urn:un:unece:uncefact:codelist:standard:UNECE:Funding Type Code: D08A
	clm69659

	20
	urn:un:unece:uncefact:codelist:standard:UNECE: EventTimeReferenceCodePaymentTermsEvent
	clm62475 Payment Terms Event

	21
	urn:un:unece:uncefact:codelist:standard:UNECE:Earned Value CalculationMethod:D08A
	clm69657

	22
	urn:un:unece:uncefact:codelist:standard:UNECE:DocumentStatus Code:D08A
	clm61373

	23
	urn:un:unece:uncefact:codelist:standard:UNECE:AdjustmentReasonDescription Code:D08A
	clm64465

	24
	urn:un:unece:uncefact:codelist:standard:UNECE:Document Name Code:D08A
	clm61001

	25
	urn:un:unece:uncefact:codelist:standard:UNECE:DeliveryTerms Coe:D08A
	clm64053

	26
	urn:un:unece:uncefact:codelist:standard:UNECE:CostManagement Code:D08A
	clm69653

	27
	urn:un:unece:uncefact:codelist:standard:UNECE:DutyorTaxorFeeCategory Code:D08A
	clm65305

	28
	urn:un:unece:uncefact:codelist:standard:UNECE:Document Name Code BillingDocument:D08A
	clm61001 Billing Document

	29
	urn:un:unece:uncefact:codelist:standard:UNECE:CostReporting Code:D08A
	clm69655

	30
	urn:un:unece:uncefact:codelist:standard:UNECE:HierarchicalStructureTypeCode:D08A
	clm69661

	31
	urn:un:unece:uncefact:codelist:standard:UNECE:ContractTypeCode:D08A
	clm69651

	32
	urn:un:unece:uncefact:codelist:standard:UNECE:DutyTaxFeeTypeCode:D08A
	clm65153

	33
	urn:un:unece:uncefact:codelist:standard:UNECE: EventTimeReferenceCode:D08A
	clm62475

	34
	urn:un:unece:uncefact:codelist:standard:UNECE:MeasurementUnitCommonCodeDuration:4
	clm6Recommendation20Durati on

	35
	urn:un:unece:uncefact:identifierlist:standard:5:ISO316612A:SecondEdition2006VI-3
	ids5IS0316612A

	36
	urn:un:unece:uncefact:codelist:standard:IANA:MIMEMediaType:2008-l 1-12
	clmlANAMIMEMediaType

	37
	urn:un:unece:uncefact:codelist:standard:IANA:CharacterSetCode:2007-05-14
	clmlANACharacterSetCode

	38
	urn:un:unece:uncefact:codelist:standard:6:0133:40106
	clm60133

	39
	urn:un:unece:uncefact:codelist:standard:5:ISO42173A:2008-ll-12
	34	clm5IS042173A

	40
	urn:un:unece:uncefact:codelist:standard:6:Recommendation20:5
	clm6Recommendation20

	41
	urn:un:unece:uncefact:data:standard:UnqualifiedDataType:6
	udt




Table B2
Requisite composition of an electronic document (data) structure
«Information about certificate of origin» (Certificate)

	Requisite name
	Requisite description /
Mandatory or optional
	Data type *
	Reason of inclusion
	Form section
	Mult.

	RootDocument
	Certificate data
	ds:RootDocumentType
	
	
	1

	1
	CancellationDateTime
	Date of the certificate annulment Optional

	ds:RootDocumentIssueDateTimeType Format - an..17. UNTDID 2379 = 304 CCYYMMDDHHMMSSZZZ
Z=Time zone
	Appendix A Tab A1 line 6
	Absent at form
	0..1


	2
	EffectiveDateTime
	Date of certificate information
change
Optional
	dsiRootDocumentEffectiveDateTimeT 
yp
Format - an..17. UNTDID 2379 = 304
CCYYMMDDHHMMSSZZZ 
Z=Time zone
	Appendix A Tab A1 line7
	Absent at form
	0..1

	3
	ExpirationDateTime
	Expiration date of the certificate Mandatory

	ds:RootDocumentExpirationDateTime
Type
Format - an..17. UNTDID 2379 = 304
CCYYMMDDHHMMSSZZZ 
Z=Time zone
	Appendix A Tab A2 line 4
	Absent at form
	1

	4
	FunctionCode
	Function code:
Mandatory
One of the values is specified:
ORG - the issued certificate of origin
is the original;
DBL - the issued certificate of origin
is the duplicate of the certificate of
origin;
CHG - the certificate of origin is issued in substitution of the original 
	ds:RootDocumentFunctionCodeType Format - an..3. EDIFACT codes (1225)
	
Appendix A Tab A1 line2
	5
	1

	5

	FunctionalReferenceID
	Certificate unique identifier Optional
	ds:RootDocumentFunctionalReferenceI
DType
Format - an..35
	Appendix A Tab A2 line 2
	4
	0.1

	6
	ID
	Registration number of the certificate Mandatory
	ds:RootDocumentIdentificationIDType
Format–an.35
	Appendix A Tab A2 line 1
	4
	1

	7
	IssueDateTime
	Date of certificate issue Mandatory
	ds:RootDocumentIssueDateTimeType
Format - an..17. UNTDID 2379 = 304 CCYYMMDDHHMMSSZZZ 
Z=Time zone
	Appendix  A Tab A1 line 3
	12
	1

	8
	issueLocationID
	Place of certificate issue Mandatory
	ds:RootDocumentIssueLocationIdentif icationIDType
Format - an..5 UN/LOCODE
	Appendix  A Tab A1 line 4
	12
	1

	9
	Type Code
	Type of the certificate, coded…
Mandatory
Fixed value «EAV»
	ds:RootDocumentTypeCode Type 
Format–an..3

	Appendix  A Tab A1 line 1
	4
	1

	10
	AdditionalDocument

	Additional Information
	Defined by the types of nesting
elements
	see lines 11-46
	see lines 11-46
	1

	11
	
	IssueDateTime
	Application Date Mandatory
	ds:AdditionalDocumentIssueDateTime
Type 
Format - an..17. UNTDID 2379 = 304
CCYYMMDDHHMMSSZZZ
Z=Time zone

	Appendix A Tab A1 line 13
	13
	1

	12
	
	issueLocationID
	Application Place, coded
Mandatory
	ds:AdditionalDocumentIssueLocationI dentificationIDType Format - an..5 UN/LOCODE
	Appendix A Tab A1 line 13
	Absent at form
	1

	13
	
	IssueLocationName
	Application Place Mandatory
	ds:AdditionalDocumentIssueLocation
NameTextType 
Format - an..256
	Appendix A Tab AI line 13
	13
	1

	14
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsilanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0.1

	15
	
	Authenticator
	Information about the authorized
body that issued the certificate
15 Mandatory
	Defined by the types of nesting elements

	Appendix A Tab AI line 11
	12
	1

	16
	
	
	Name
	Name of the authorized body that
issued the certificate Mandatory
	ds:AuthenticatorNameTextType
Format - an..70
	Appendix A Tab AI line 11
	12
	1

	17
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0.1

	18
	
	
	ID
	Identifier of the authorized body that issued (authenticated) the certificate Mandatory
	ds:AuthenticatorIdentificationIDType
Format - an..17. International codes
(e.g. DUNS, EAN) or user codes
	Appendix A Tab A1 line 11
	Absent at form
	1

	19
	
	
	RoleCode
	RoleCode of the authorized body that issued (authenticated) the certificate Mandatory Fixed value AX.
	ds:AuthenticatorRoleCodeType
Format - an..3. UNTDID 3035 = AX,
Authenticating party
	-
	Absent at form
	1

	20
	
	
	Address
	Address Data of authorized body that issued (authenticated) the certificate
Mandatory
	Defined by the types of nesting
elements
	Appendix A Tab A1 line 11
	12
	1

	21
	
	
	
	TypeCode
	Address type code
Optional
	ds:AddressTypeCodeType Format - an..3. EDIFACT codes
(3131)
	-
	Absent at form
	0.1

	22
	
	
	
	CityName
	City name, city 
Optional
	ds:AddressCityNameTextType
Format - an..35
	Appendix A Tab A1 line 11
	12
	0.1

	23
	
	
	
	
	@ languageID
	Language identifier Optional
«En» by Default

	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc- 
editor.org/rfc/rfc5646.txt
	-
	-
	0.1

	24
	
	
	
	CountryCode
	Country code according to ISO
3166
Certificate issued country code.
Mandatory
	ds:AddressCountryCodeType
Format - a2.EDIFACT codes (3207) =
ISO 3166-1 2-alpha code

	Appendix A Tab A1 line 4 and 11
	4
	1

	25
	
	
	
	CountrySubDivision 
Code
	Code of the country subdivision Optional

	ds:AddressCountrySubDivisionCodeType
Format - an..9. EDIFACT codes (3229)
 = ISO 3166-2 2-alpha code or User code
	Appendix A Tab A1 line 11
	12
	0.1

	26
	
	
	
	CountrySubDivision Name
	Name of the country subdivision Optional
	ds:AddressCountrySubDivisionNameT
extType
Format - an..35
	Appendix A Tab A1 line 11
	12
	0.1

	27
	
	
	
	
	@ languageID
	Language identifier Optional
«En» by Default

	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc- 
editor.org/rfc/rfc5646.txt
	-
	-
	0.1

	28
	
	
	
	
	Line
	Building number and street name, or P/О Box Building number
Optional
	ds:AddressLineTextTуpe 
Format - an..70
	Appendix A Tab A1 line    13


	Appendix A Tab A1 line    13-

	0..1


	29
	
	
	
	
	@ languageID
	Language identifier Optional
«En» by Default

	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc- 
editor.org/rfc/rfc5646.txt
	-
	-
	0.1

	30
	
	
	
	PostcodelD
	Post code
Optional
	ds:AddressPostcodeIDType 
Format - an..9
	Appendix A Tab A1 line 11
	12
	0.1

	31
	
	LPCOAuthorizedParty
	Applicant data
 Mandatory
	Defined by the types of nesting elements 
	Appendix A Tab A1 line 13
	13
	1

	32
	
	
	Name
	Applicant Name 
Mandatory
	ds:LPCOAuthorizedPartyNameTextType
Format - an..70
	Appendix A Tab A1 line 13
	13
	1

	33
	
	
	
	@ languageID		
	Language identifier 
Optional
«En» by Default
	xsdanguage 
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	34
	
	
	ID
	Identifier of the applicant Optional
 
	dsiLPCOAuthorizedPartyldentification
IDType
Format - an..17. International codes
(e.g. DUNS, EAN) or user codes
	-
	Absent at form
	0..1

	35
	
	
	RoleCoae	
 

	RoleCode of the body that issued (authenticated) the certificate Mandatory
Fixed value - DT.
	dsiLPCOAuthorizedPartyRoleCodeType
Format - an 3. UNTDID 3035 = DT,
Declarant

	-
	Absent at form
	1

	36
	
	
	Address		

	Applicant Address Data
Mandatory
	Defined by the types of nesting
elements
	Appendix A Tab A1 line 13
	13

	1

	37
	
	
	
	TypeCode	

	Address type code
Optional
	ds:AddressTypeCodeType Format - an..3. EDIFACT codes (3131)
	-
	Absent at form
	0..1

	38
	
	
	
	City Name
	City Name city Optional
	ds:Address Type City Name Text Type Format - an..35
	Appendix A Tab A1 line 13
	13
	0..1

	39
	
	
	
	
	@ languageID
	Language identifier Optional
«En» by Default

	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc- 
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	40
	
	
	
	CountryCode
	Country code according to ISO
3166 Mandatory
	ds:AddressCountryCodeType
Format - a2.EDIFACT codes (3207) = ISO 3166-1 2-alpha code

	Appendix A Tab A1 line 13
	13
	1

	41
	
	
	
	CountrySubDivision Code
 

	Code of the country subdivision Optional

	ds:AddressCountrySubDivisionCodeType
Format - an..9. EDIFACT codes 
(3229) = ISO 3166-2 2-alpha code or 
User code
	Appendix A Tab A1 line 13
	13
	0..1

	42
	
	
	
	CountrySubDivision Name
	Name of the country subdivision Optional

	ds:AddressCountrySubDivision Name T      extType
Format - an..35
	Appendix A Tab A1 line 13
	13
	0..1

	43
	
	
	
	
	@ languageID
	Language identifier 
Optional
«En» by Default

	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc- 
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	44
	
	
	
	Line
	Building number and street name, or P/О Box Building number
Optional
	ds:AddressLineTextTуpe 
Format - an..70
	Appendix A Tab A1 line    13


	Appendix A Tab A1 line    13-

	0..1


	45
	
	
	
	
	@ languageID
	Language identifier 
Optional
«En» by Default

	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc- 
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	46
	
	
	
	PostcodelD	
	


	Post code 
Optional
	ds:AddressPostcodeIDType
Format - an..9
	Appendix A Tab A1 line 13
	Appendix A Tab A1 line 13-

	0..1

	47
	Additionallnformation
	Special Marks 
Mandatory
	Defined by the types of nesting elements  
	Appendix A Tab A 1 line 8, 15
	see lines 48-52
	1..*

	48
	
	Content	

	Additional Information description
in free form.
Optional 
Used for transmitting the transfer of information about the certificate issued retroactively (provided that the value is specified in the Statement Code – R.TR)
	ds:AdditionalInformationContentText 
Type
Format - an..512
	Absent at form
	Appendix A Tab A1 line 8,
15

	0..1

	49
	
	StatementCode
	Type code for tha additional information: “R.DT” for data registration date-time in authorized body database, “R.TR” if the certificate was isuued retroactively/ Mandatory
	ds:AdditionalInformationStatementCo
deType
Format - an..17, User codes
	Appendix A Tab Ai line 8, 15

	Absent at form for»R.DT», Section 5 for «R.TR»
	1

	50
	
	StatementDescription		
	StatementCode description in free- 
form.,,
Mandatory
	ds:AdditionalInformationStatementDe
scriptionTextType	
Format - n.,512
	Appendix A Tab Al line 8, 15
	Absent at form
	0..1

	51
	
	
	@ languageID
	Language identifier 
Optional
«En» by Default

	Appendix A Tab Al line 8, 15
	-
	-
	0...1

	52
	
	LimitDateTime	
	Certificate data registration date- time in authorized body database Mandatory for StatementCode
«R.DT», prohibited (0) для
StatementCode «R.TR»,
	ds:AdditionalInformationLimitDateTi
meType
Format - an..17. UNTDID 2379 = 304
CCYYMMDDHHMMSSZZZ
Z=Time zone
	Appendix A Tab A1 line 15
	Absent at form
	0..1

	53
	GoodsShipment
	Goods shipment
Mandatory
	Defined by the types of nesting
elements
	Appendix A Tab A4
	6-11
	1

	54
	
	ExportationCountryCode	

	Origin country code according to
ISO 3166
Mandatory
	ds:GoodsShipmentExportationCountry CodeType
Format - a2.EDIFACT codes (3207) =
ISO 3166-1 2-alpha code
	Appendix A Tab A 1 line 10
	13
	1

	55
	
	Additionallnformation

	Additional iformation on invoice
issued in the Third Country
Optional
	Defined by the types of nesting elements
	Appendix A Tab A5 line 2
	8
	0..*

	56
	
	
	Content	

	Data required:
Name and the country of the company which issued the invoice; information that the invoice will be issued later, as well as the trade name and the address of a physical person or a legal entity which will issue this invoice in the third country.
Mandatory)
	ds:AdditionalInformationContentText
Type
Format - an..512
	Appendix A Tab A5 line 2
	8
	1

	57
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	58
	
	
	StatementCode
	Type code for tha additional information: Invoice is issued in the third  country
Mandatory
Fixed value = «TCI»
	ds:AdditionalInformationStatementCo
deType
Format - an..17, User codes
	Appendix A Tab A5 line 2

	8
	1

	59
	
	
	StatementDescription		
	StatementCode description in free- 
form.,,
Mandatory
	ds:AdditionalInformationStatementDe
scriptionTextType	
Format - n.,512
	Appendix A Tab A5 line 2
	Absent at form
	0..1

	60
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	61
	
	Consignee	
	Information about Consignee Optional
	Defined by the types of nesting elements
	Appendix A Tab A3 line3
	2
	0..1

	62
	
	
	Name	

	Name of Consignee
Mandatory
	ds:ConsigneeNameTextType
Format - an..70
	Appendix A Tab A3 line3
	2
	1

	63
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	64
	
	
	ID
	Consignee Identifier Optional

	ds:ConsigneeIdentificationIDType Format - an..17. International codes (e.g. DUNS, EAN) or user codes
	-
	Absent at form
	0..1

	65
	
	
	RoleCode	

	Consignee RoleCode
Mandatory 
Fixed value - CN.
	ds:ConsigneeRoleCodeType
Format - an..3. UNTDID 3035 = CN
	-
	Absent at form
	1

	66
	
	
	Address	

	Consignee address data
Mandatory
	The element has an element content	
	Appendix A Tab A3 line 3
	2
	1

	67
	
	
	
	TypeCode	

	Address type code
Optional
	ds:AddressTypeCodeType Format - an..3. EDIFACT codes (3131)
	-
	Absent at form
	0..1

	68
	
	
	
	CityName	

	City name, city
Optional
	ds:AddressCityNameTextType
Format - an..35
	Appendix A Tab A3 line 3
	2
	0..1

	69
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	70
	
	
	
	CountryCode
	Country code according to ISO
3166 
Mandatory
	ds:AddressCountryCodeType
Format - a2.EDIFACT codes (3207) = ISO 3166-1 2-alpha code
	Appendix A Tab A3 line 3
	2
	1

	71
	
	
	
	CountrySubDivision
Code


	Code of the country subdivision
Optional
	ds:AddressCountrySubDivisionCodeT 
ype
Format - an..9. EDIFACT codes (3229) = ISO 3166-2 2-alpha code or User code
	Appendix A Tab A3 line 3
	2
	0..1

	72
	
	
	
	
	CountrySubDivision
Name

 
	Name of the country subdivision
Optional

	ds:AddressCountrySubDivisionNameT
extType
Format - an..35
	Appendix A Tab A3 line 3
	2
	0..1

	73
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	74
	
	
	
	Line		
	Building number and street name, or
P/О Box Building number 
Optional
	ds:AddressLineTextType Format - an..70

	Appendix A Tab A3 line 3
	2
	0..1

	75
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	76
	
	
	
	PostcodelD
	

	Post code 
Optional
	ds:AddressPostcodeIDType 
Format - an..9
	Appendix A Tab A3 line 3
	2
	0..1

	77
	
	
	Contact
	Data on Consignee contact persons Optional
	Defined by the types of nesting 
elements
	-
	Absent at form
	0..*

	78
	
	
	
	Name
	Contact person»s name
Optional

	ds:ContactNameTextType 
Format - an..70
	-
	Absent at form
	0..1

	79
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	80
	
	
	
	Communication	
	
	Information about communication
channels Optional
	Defined by the types of nesting elements
	-
	Absent at form
	0..*

	81
	
	
	
	
	ID
	Communication link identifier -phone number, e-mail address etc.Mandatory
	ds:CommunicationIdentificationIDType
Format - an 50
	-
	Absent at form
	0..1

	82
	
	
	
	
	Type ID
	Communication link type: codefrom EDIFACT Codelist 3155 
Optional
	ds:CommunicationTypeIDType
Format - an..3. EDIFACT codes 
(3155)
	-
	Absent at form
	0..1

	83
	
	Consignment
	Route and transport details
Optional
	Defined by the types of nesting
elements
	Appendix A Tab A3 line 4
	3
	0..*

	84
	
	
	Border Transport Means
	Information about transport means
Optional
	Defined by the types of nesting
elements
	Appendix A Tab A3 line 4
	3
	0..1

	85
	
	
	
	Name
	Border Transport Means Name
Optional
	ds:ВorderTransportMeansNameTextType Format - an..35
	Appendix A Tab A3 line4
	3
	0..1

	86
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	87
	
	
	
	ID
	Transport means identifier Optional For the road transport – national registration numbers; 
For the railway transport - registration numbers of vans (platforms, tanks etc);
For the sea ( maritime) transport -
name of a vessel;
For the air transport - flight number
	ds:BorderTransportMeansIdentificatio nIDType
Format - an..25
	Appendix A Tab A3 line4
	3
	0..1

	88
	
	
	
	TypeCode
	Transportation mode code: Mandatory
To be filled in:
by the authorities of the EAEU in accordance with the classifier of modes of transport and transportation of goods used in the Union;
by the authorities of Viet Nam in accordance with the classifier of modes of transport and transportation of goods used in Viet
Nam
	ds:ВorderTransportMeansTypeCodeType
Format - an 2
See Table C3
			

	Appendix A Tab A3 line 4
	3
	1

	89
	
	
	
	
	@ ListAgencyName	

	Responsible organization
Mandatory
Values: EAEU, Viet Nam
	clm63055:AgencyIdentificationCode ContentType
Format - an 18
	-
	-
	1

	90
	
	
	LoadingLocation
	
	Loading Location Data Optional
	Defined by the types of nesting elements
	Appendix A Tab A3 line 4
	3
	0..*

	91
	
	
	
	Name
	Loading Location Name
Mandatory
	ds:LoadingLocationNameTextType
an.256
	Appendix A Tab A3 line 4
	3
	1

	92
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	93
	
	
	
	ID
	Loading Location Name, coded Mandatory
	ds:LoadingLocationIdentificationIDType Format - an..5 UN/LOCODE
	Appendix A Tab A3 line 4
	3
	1

	94
	
	
	
	DepartureDateTime	
	DepartureDateTime Optional
	ds:LoadingLocationDepartureDateTime
Type Format - an..17.UNTDID2379 = 304
CCYYMMDDHHMMSSZZZ
Z=Time zone
	Appendix A Tab A3 line 4
	3
	0..1

	95
	
	
	UnloadingLocation		
	Unloading Location Data
Optional

	Defined by the types of nesting elements 

	Appendix A Tab A3 line 4
	3
	0..*

	96
	
	
	
	ID
	Unloading Location Name, coded Mandatory
	ds:UnloadingLocationIdentificationID 
Type
Format - an..5 UN/LOCODE
	Appendix A Tab A3 line 4
	3
	1

	97
	
	DeliveryDestination	
	

	Certificate destination country code
Mandatory

	Defined by the types of nesting elements

	Appendix A Tab A1 line 5
	4
	1

	98
	
	
	Address
	Certificate destination country code
Mandatory
	Defined by the types of nesting elements
	Appendix A Tab A1 line 5
	4
	1

	99
	
	
	
	CountryCode	
	
	Code of country certificate to be
submitted, according to ISO 3166
Mandatory
	ds:AddressCountryCodeType
Format - a2. EDIFACT codes (3207)
= ISO 3166-1 2-alpha code 
	Appendix A Tab A1 line 5
	4
	1

	100
	
	Exporter
	Exporter Data
Mandatory

	Defined by the types of nesting elements
	Appendix A Tab A3 line 1
	1
	1

	101
	
	
	Name
	Exporter Name
Mandatory
	ds:ExporterNameTextType
an..70
	Appendix A Tab A3 line 1
	1
	1

	102
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	103
	
	
	ID
	Exporter Identifier
Optional
	ds:ExporterIdentificationIDType Format - an..17. International codes
(e.g. DUNS, EAN) or user codes
	-
	Absent at form
	1

	104
	
	
	RoleCode	
	

	Exporter RoleCode
Mandatory 
Fixed value EX.
	ds:ExporterRoleCodeType
Format - an..3. UNTDID 3035 = EX
	-
	Absent at form
	1

	105
	
	
	Address
	Exporter Address Data
Mandatory
	Defined by the types of nesting elements

	Appendix A Tab A3 line 1
	1
	0..1

	106
	
	
	
	TypeCode

	Address type code
Optional
	ds:AddressTypeCodeType Format - an..3. EDIFACT codes (3131)
	-
	Absent at form
	0..1

	107
	
	
	
	CityName	

	City name, city
Optional
	ds:AddressCityNameTextType
Format - an..35
	Appendix A Tab A3 line 1
	1
	0..1

	108
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	109
	
	
	
	CountryCode	
 
	
	Country code according to ISO
3166 
Mandatory
	ds:AddressCountryCode
TypeFormat – a2. EDIFACT codes (3207) =
ISO 3166-1-2-alpha code
	Appendix A Tab A3 line 1
	1
	1

	110
	
	
	
	Country Sub Division Code
	Code of the country subdivision Optional

	ds:AddressCountry Sub Division Code Type
Format – an.9. EDIFACT codes (3229) =
ISO 3166-2-2-alpha code or User code
	Appendix A Tab A3 line 1
	1
	0..1

	111
	
	
	
	Country Sub Division Name
	Name of the country subdivision Optional

	ds:AddressCountry Sub Division Name T
ext Type
Format – an.35
	Appendix A Tab A3 line 1
	1
	0..1

	112
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	113
	
	
	
	Line
	Building number snd street name, or P/O Box Building number 
Optional
	ds:Address Line Text Type
Format – an.70.

	Appendix A Tab A3 line 1
	1
	0..1

	114
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	115
	
	
	
	PostcodeID
	Post code Optional

	ds:Address PostcodeID Type
Format – an.9
	Appendix A Tab A3 line 1
	1
	0..1

	116
	
	Government Agency Goodsl tem
	Data on goods Mandatory

	Defined by the types of nesting elements
	Appendix A Tab A4
	6-11
	1..*

	117
	
	
	Seguence Numeric
	Seguence Numeric Mandatory

	ds.Commodity Seguence Numeric Type Format – n..5
	Appendix A Tab A4 line 1
	6
	1

	118
	
	
	Commodity
	Description of good at line Mandatory
	Defined by the types of nesting elements
	Appendix A Tab A4 line 1
	8
	1

	119
	
	
	
	Description
	General description of good at line Mandatory
	ds.Commodity Description Text Type
an..512
	Appendix A Tab A4 line 4
	8
	1

	120
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	- Appendix A Tab A4 line 4
	-
	0..1

	121
	
	
	
	CountQuanlity
	Cood Quanlity at line Optional

	ds.Commodity CountQuanlity Type
Format – n..16
	Appendix A Tab A4 line 7
	10
	0..1

	122
	
	
	
	
	@unit Code
	Units of measurement Mandatory
	Clm6Recommendation 20:Measurement Unit Common Code Content Type
Format - an..5.International codes for Union,National code for Viet Nam See Table C2
	Appendix A Tab A4 line 7
	10
	1

	123
	
	
	
	Additionallnformaion
	Infoirmation on additional marks,
FTA:
If the goods satisfy a description of footwear made of leather for use in indoor and outdoor sporting activities (ex 6403 91, 6403 99) stipulated in Annex 1 to this Agreement the mark «Sporting Footwear» shall be indicated.
Optional
	Defined by the types of nesting elements

	Appendix A Tab A4 line 5
	8
	0..*

	124
	
	
	
	
	Content

	Additional Information (additional marks) description in free form. Optional
	ds:AdditionalInformaticnContentText
Type
Format - an..512
	-
	Absent at form
	0..1

	125
	
	
	
	
	StatementCode	

	Additional marks, coded
Fixed value: «Sporting Footwear»
Mandatory	
	ds:AdditionalInformationStatementCo
deType
Format - an..17, User codes= Sporting
Footwear.

	Appendix A Tab A4 line 5
	8
	0..1

	126
	
	
	
	
	StatementDescription
 

	Additional marks. Free text .Marked 
as «Sporting Footwear»
Optional 

	ds:AdditionalInformationStatementDe scriptionTextType
Format - li..512


	Appendix A Tab A4 line 5
	8
	0..1

	127
	
	
	
	
	
	@ languageID 
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	- Appendix A Tab A4 line 4
	-
	0..1

	128
	
	
	
	Classification	
	Commodity code data Mandatory
	Defined by the types of nesting elements


	Appendix A Tab A4 line 3
	8
	1

	129
	
	
	
	
	ID	

	Commodity code according to the line. 6-digits HS code according to
The Harmonized Commodity Description and Coding System/
Mandatory
	ds:ClassificationIdentificationIDType
Format - an..18
	Appendix A Tab A4 line 3
	8
	1

	130
	
	
	
	
	IdentificationTy
peCode
	Commodity code type
Fixed value «ZZZ» - Mutually
defined
Mandatory
	ds:ClassificationIdentificationTypeCo
deType
Format - an..3, EDIFACT codes
(7143)
	-
	Absent at form
	1

	131
	
	
	
	GoodsMeasure	
 

	

	Goods weight data by line
Optional

	Defined by the types of nesting
elements

	Appendix A Tab A4 line 7
	10
	0..1

	132
	
	
	
	
	GrossMassMeas 
 ure
		

	Goods gross weight with units of 
measurment specification
Mandatory

	ds:GoodsMeasureGrossMassMeasureType
Format - n.. l 6,6

	Appendix A Tab A4 line 7
	10
	1

	133
	
	
	
	
	
	@unit Code
	Units of measurement Mandatory
	Clm6Recommendation 20:Measurement Unit Common Code Content Type
Format - an..5.International codes for Union,National code for Viet Nam See Table C2
	Appendix A Tab A4 line 7
	10
	1

	134
	
	
	
	
	NetNetWeight
Measuree
 
	Goods Net weight with units of measurment specification Optional
	ds:GoodsMeasureNetNetWeightMeasu
reType
Format - n.. l 6,6
	Appendix A Tab A4 line 7
	10
	1

	135
	
	
	
	
	
	@unit Code
	Units of measurement Mandatory
	Clm6Recommendation 20:Measurement Unit Common Code Content Type
Format - an..5.International codes for Union,National code for Viet Nam See Table C2
	Appendix A Tab A4 line 7
	10
	1

	136
	
	
	
	
	Product Name
	Additional good data bn line
Optional
	Defined by the types of nesting elements 

	Appendix A Tab A4 line 4
	8
	0,,*

	137
	
	
	
	
	Name
	Good Name or other product
characteristic
	ds:ProductNameNameTextType Format - an..35
	Appendix A Tab A4 line 4
	8
	1

	138
	
	
	
	
	
	@ languageID 
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	- Appendix A Tab A4 line 4
	-
	0..1

	139
	
	
	
	
	NameQualifierCode
 
		

	A qualifier to describe the  
commodity name or other product characteristic, e.g., chassis No for motor vehicles/ Optional
	ds:ProductNameNameQualifierCodeType
Format - an..3. EDIFACT codes
(7081)

	Appendix A Tab A4 line 4
	8
	0..1

	140
	
	
	Origin	
	Origin criteria Mandatory
	Defined by the types of nesting elements	

	Appendix A Tab A4 line 6
	12
	1

	141
	
	
	
	RuleCode
	Origin criteria:Mandatory
WO - goods are wholly obtained or produced in a Party as provided for in article 4.4 of Free Trade Agreement (hereinafter referred to as FTA);
PE - goods are produced entirely in the territory of one or both Parties, exclusively from originating materials from one or both Parties; PSR - goods are produced in the
territory of a Party using non-
originating material and satisfies the
requirements as specified in Annex
3 to FTA
	ds:OriginRuleCodeType
Format - an..3. User codes
	Appendix A Tab A4 line 6
	9
	1

	142
	
	
	Packaging
	Packaging data
Mandatory
	Defined by the types of nesting elements
	Appendix A Tab A4 line 2
	7
	1. *

	143
	
	
	
	MarksNumbersID	

	Free form description of the marks
and numbers on a transport unit or package.
Optional
	ds:PackagingMarksNumbersIDType
Format - an..512 UN/ECE
Recommendation 15
	Appendix A Tab A4 line
	7
	0..1

	144
	
	
	
	QuantityQuantity	

	Package quantity
Mandatory
	ds:PackagingQuantityQuantityType Format - n..l 6,6
	Appendix A Tab A4 line
	7
	1

	145
	
	
	
	TypeCode	

	Package type
Mandatory
	ds:PackagingTypeCodeType Format - an..2. EDIFACT codes (7065) = UN/ECE Recommendation
21 Annex VI
	Appendix A Tab A4 line
	7
	1

	146
	
	Importer	

	Importer Data
Mandatory
	Defined by the types of nesting elements
	Appendix A Tab A3 line 2
	2
	1

	147
	
	
	Name
	Importer Name
Mandatory
	ds:ImporterNameTextTvpe an..70
	Appendix A Tab A3 line 2
	2
	1

	148
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default	

	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt		
	-
	-
	0..1

	149
	
	
	ID
	Importer Identifier
Optional
	ds:ExporterIdentificationIDType
Format - an..17. International codes
(e.g. DUNS, EAN) or user codes
	-
	Absent at form
	0..1

	150
	
	
	RoleCode	

	Importer RoleCode
Mandatory
Fixed value - IM.
	dsrlmporterRoleCodeType
Format - an..3. UNTDID 3035 = IM
	-
	Absent at form
	0..1

	151
	
	
	Address	

	Importer address data
Mandatory
	Defined by the types of nesting elements
	Appendix A Tab A3 line 2
	2
	1

	152
	
	
	
	TypeCode	

	Address type code
Optional
	ds:AddressTypeCodeType
Format - an..3. EDIFACT codes
(3131)
	-
	Absent at form
	0..1

	153
	
	
	
	CityName	

	City name, city
Optional
	ds:AddressCityNameTextType
Format - an..35
	Appendix A Tab A3 line 2
	2
	0..1

	154
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default		
			
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	155
	
	
	
	CountryCode	

	Country code according to ISO
3166 Mandatory
	ds:AddressCountryCodeType
Format - a2.EDIFACT codes (3207) = ISO 3166-1 2-alpha code
	Appendix A Tab A3 line 2

	2
	1

	156
	
	
	
	CountrySubDivision
Code
	Code of the country subdivision
Optional
	ds:AddressCountrySubDivisionCodeT ype
Format - an..9. EDIFACT codes (3229) = ISO 3166-2 2-alpha code or User code
	Appendix A Tab A3 line 2
	2
	0..1

	157
	
	
	
	CountrySubDivision Name  	

	Name of the country subdivision
Optional

	ds:AddressCountrySubDivisionNameT
extTvpe
Format - an..35
	Appendix A Tab A3 line 2
	2
	0..1

	158
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
			
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	159
	
	
	
	Line	

	Building number and street name, or
P/О Box Building number
Optional
	ds:AddressLineTextType
Format - an..70
	Appendix A Tab A3 line 2
	2
	0..1

	160
	
	
	
	
	@ languageID
	Language identifier
Optional
«En» by Default	
	
			
	xsdanguage
Format - an..35. IETF RFC 5646
http://www.rfc-
editor.org/rfc/rfc5646.txt
	-
	-
	0..1

	161
	
	
	
	PostcodelD
	Post code 
Optional
	ds:AddressPostcodelDType 
Format - an..9
	Appendix A Tab A3 line 2
	2
	0..1

	162
	
	Invoice	
	Invoice data 
Mandatory	
	Defined by the types of nesting
elements
	Appendix A Tab A4 line 8

	11
	1..*

	163
	
	
	ID
	Invoice number by line 
Mandatory
	ds:InvoiceIdentificationIDType
Format -an..35
	Appendix A Tab A5 line 1
	11
	1

	164
	
	
	IssueDateTime	

	Invoice issue date by line
Mandatory
	dsiInvoicelssueDateTimeType
Format - an..17. UNTDID 2379 = 304
CCYYMMDDHHMMSSZZZ
Z=Time zone
	Appendix A Tab A5 line 1
	11
	1

	165
	
	
	TypeCode
	Invoice Type by line, including invoice, issued by Exporter, invoice, isssued in third-country (TCI).
Mandatory
	ds:InvoiceTypeCodeType Format - an..3. EDIFACT codes (1001) or National codes
	Appendix A Tab A5 line 1
	11
	1

	166
	
	
	SequenceNumeric	

	Sequence number. It has to correlate
with the GovernmentAgency Goodsltmem element SequenceNumeric .
Mandatory
	ds:InvoiceSequenceNumericType
Format - n..5
	Appendix A Tab A5 line 1
	6
	1

	167
	PreviousDocument	

	Identification of previous
certificates Optional
	Defined by the types of nesting
elements

	Appendix A Tab A1 line 9
	5
	0..*

	168
	
	ID	

	Registration number of the certificate
Mandatory
	ds:PreviousDocumentIdentificationID 
Type
Format - an..35
	Appendix A Tab A1 line 9
	5
	1

	169
	
	IssueDateTime	

	Registration date of the certificate
Mandatory
	ds:RootDocumentIssueDateTimeType Format - an..17. UNTDID 2379 = 304 CCYYMMDDHHMMSSZZZ
Z=Time zone
	Appendix A Tab A1 line 9
	5
	1

	170
	
	TypeCode	

	Certificate of origin type code
Mandatory
 Fixed value - 861
	ds:RootDocumentTypeCodeType Format - an..3. EDIFACT codes (1001) or National codes=861
	-
	Absent at form
	1


	



Table B3
Requisite composition of an electronic document (data) structure «Notification on absence of information» (Response)

	Requisite name
	Requisite description
	Data type *
	Mult.


	RootDocument
	Notification of the results of processing of
information
	ds:RootDocumentType
	1

	1
	IssueDateTime
	Date and time of notification 
Optional
	ds:RootDocumentIssueDateTimeType
Format: an..17 Source: UNTDID 2379 = 304 CCYYMMDDHHMMSSZZZ
Z=Time zone
	0..1

	2
	Additionallnformation

	Description of the result of information processing in a free form 
Optional
	Defined by the types of nesting elements
	0..*

	3
	
	StatementDescription

	Description text, up to 512 symbols Mandatory (1 )
	ds:AdditionalInformationStatementDescriptionTextTyp
Format - an 512
	1

	4
	
	
	@ languageID
	Language identifier
Optional
«En» by Default
	xsdanguage
Format - an..35. IETF RFC 5646 http://www.rfc-
editor.org/rfc/rfc5646.txt
	0..1

	5
	ContactOffice
	Contact information
Optional
	Defined by the types of nesting elements
	0..1

	6
	
	Contact
	Contact person
Optional
	Defined by the types of nesting elements
	0..*

	7
	
	
	Name	

	Contact person»s name
Mandatory
	ds:ContactNameTextType 
Format: an..70
	1

	8
	
	
	
	@ languageID	

	Language identifier
Optional
«En» by Default
	xs:danguage
Format - an..35. IETF RFC 5646 http://www.rfc-
editor.org/rfc/rfc5646.txt,
IANA Language Subtag Registry http://www.iana.org/assigments/languege - subtag -registry
	0..1

	9
	
	
	Communication
	Information about communication links
Mandatory
	Defined by the types of nesting elements
	1..*

	10
	
	
	
	ID
	Communication link identifier Mandatory
	ds:CommunicationIdentificationIDType Format: an..50
	1

	11
	
	
	
	TypelD
	Communication link type: code from EDIFACT
Codelist 3155
Optional
	ds:CommunicationTypelDType Format: an..3
Source: EDIFACT codes (3155)

	0..1

	12
	
	Communication
	Information about communication links
Optional
	
	0..*

	13
	
	
	ID 

	Communication link identifier
Mandatory
	ds:CommunicationIdentificationlDType
Format: an..50
	1

	14
	
	
	TypelD
	Communication link type: code from EDIFACT
Codelist 3155 Optional
	ds:CommunicationTypeIDType
Format: an..3
Source: EDIFACT codes (3155)
	0..1

	15
	Error	

	Validation error
Optional
	Defined by the types of nesting elements
	0..*

	16

	
	ValidationCode	

	Error code
Mandatory
	ds:ErrorValidationCodeType	
Foramt an 3. WCO codes or user codes
	1

	17

	
	
	@ name
	Error message text
Optional
	xs:string
	0..1

	18

	
	Pointer	 

	Error location
Optional
	Defined by the types of nesting elements
	0..*

	19
	
	
	SequenceNumeric	

	Sequence number
Mandatory
	ds:PointerSequenceNumericType	
Format - n 5
	1

	20
	
	
	TagID	

	Data element tag identifier
Mandatory
	ds:PointerTagIDType	
Format - an 4
	1

	21
	Status	
	Status of processing Mandatory
	Defined by the types of nesting elements
	1

	22
	
	NameCode	
	Status code: Mandatory
0 - Data processed successfully
1 - No data available
	ds:StatusNameCodeType	
Format - n 1
	1

	23
	
	ReleaseDateTime	

	Date and time of status
Mandatory
	ds:StatusReleaseDateTimeType	
Format - an 17. UNTDID 2379 = 304 
CCYYMMDDHHMMSSZZZ  Z=Time zone
	1

	24
	Declaration
	Processed certificate transaction identifier
Optional
	Defined by the types of nesting elements
	0..1

	25
	
	FunctionalReferencelD	

	Certificate unique identifier 
Optional
	ds: DeclarationFunctionalReferencelDType 
Format - an..35
	0..1

	26
	
	ID	
	Certificate registration number 
Mandatory
	ds:RootDocumentIdentificationIDType
Format: an..35
	1



Table B4
Requisite composition of an electronic document (data) structure «Request for information about certificates of origin» (Request)

	Requisite name
	Requisite description
	Data type
	Mult.

	RootDocument

	Information about certificate
	RootDocumentType
	1

	1
	ID
	Certificate ID 
Mandatory
	ds:RootDocumentIdentificationIDType Format - an..35
	0..1

	2
	IssueDateTime	

	Date of the certificate issue or date of data update
Mandatory
	ds:RootDocumentIssueDateTimeType	
Format - an 17. UNTDID 2379 = 304
	1

	3
	IssueLocationID
 

	Country of issuance of the certificate code.
Mandatory 
UN/LOCODE data format: (first two symbols is
country code - format ISO 3166-1 alpha-2)
	ds:RootDocumentIssueLocationIdentificationIDType	
Format - an..5 UN/LOCODE
	1

	4
	TypeCode	

	Type of the certificate, coded. Fixed value «EAV»
Mandatory
	ds:RootDocumentTypeCodeType
Format - an..3
	0..1



* There are the format rules explanations:
1)	n - digit in the interval 0..9 is allowed;
2)	a - character in the intervals a-z, A-Z is allowed
3)	an - both: digit in the interval 0..9 or character in the interval a-z, A-Z is allowed
4)	ak, where k>0 - a sting of characters with length k;
an..k, where k>0 - string of characters and digits with length less than k+1.

Appendix С. W3C XML-Schemes
Table Cl
Requisite of an electronic document (information) structure «Information about
certificates of origin» (Certificate)

<?xml version- «1.0» encoding=«UTF-8»?>
<!	edited with XMLSpy v2013 spl (http://www.altova.com) by AMD (ru-Board)	>
<xs:schcma xmlns:xs=«http://www.w3.org/2001/XMLSchema»
xmlns=«um:wco:datamodel:WCO:Declaration:2» mlns:ds=«um:wco:datamodel:WCO:DS:l» 
targetNamespace=«um:wco:datamodel:WCO:Declaration:2»>
<xs:import namespace=«um:wco:datamodel:WCO:DS:1» schemaLocation- «DS_ lp0.xsd»/>
<xs:element name=«RootDocument» type=«RootDocumentType»/>
<xs:complexType name=«RootDocumentType»>
<xs:sequence>
<xs:element name=«CancellationDateTime»
type=«dsiRootDocumentCancellationDateTimeType» minOccurs=«0»/>
<xs:element name-»EffectiveDateTime» type=«ds:RootDocumentEffectiveDateTimeType»
minOccurs=«0»/>
<xs:element name=«ExpirationDateTime» Type=«ds:RootDocumentExpirationDateTimeType»/>
<xs:element name=«FunctionCode» type=«ds:RootDocumentFunctionCodeType»/>
<xs:element name=«FunctionalReferenceID»
type=«ds:RootDocumentFunctionalReferenceIDType» minOccurs=«0»/>
<xs:elcment name=«ID» type=«ds:RootDocumentIdentificationIDType»/>
<xs:element name=«IssueDateTime» type=«ds:RootDocumentIssucDateTimeType»/>
<xs:element name=«issueLocationID»
type=«ds:RootDocumentIssueLocationIdentificationIDType»/>
<xs:element name- «TypeCode» type=«ds:RootDocumentTypeCodeType»/>
<xs:element name- «AdditionalDocument»>
<xs:complexType>
<xs:sequence>
<xs:element name=«IssueDateTime» type=«ds:AdditionalDocumentIssueDateTimeType»/>
<xs:element name=«issueLocationID»
type=«ds:AdditionalDocumentIssueLocationIdentificationIDType»/>
<xs:element name=«IssueLocationName»
type=«ds:AdditionalDocumentIssueLocationNameTextType»/>
<xs:element name=«Authenticator»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:AuthenticatorNameTextType»/>
<xs:element name=«ID» type=«ds:AuthenticatorldentificationIDType»/>
<xs:element name=«RoleCode» type=«ds:AuthenticatorRoleCodeType»/>
<xs:element name=«Address»>
<xs:complexType>
<xs:sequence>
<xs:element name=«TypeCode» type=«ds:AddressTypeCodeType» minOccurs:=«0»/>
<xs:element name=«CityName» type=«ds:AddressCityNameTextType» minOccurs=«0»/>
<xs:element name=«CountryCode» type=«ds:AddressCountryCodeType»/>
<xs:element name- «CountrySubDivisionCode»
type-»ds:AddressCountrySubDivisionCodeType» minOccurs=«0»/>
<xs:element name=«CountrySubDivisionName»
type=«ds:AddressCountrySubDivisionNameTcxtType» minOccurs=«0»/>
<xs:element name=«Line» type=«ds:AddressLineTextType» minOccurs=«0»/>
<xs:element name=«PostcodeID» type=«ds:AddressPostcodeIDType» minOccurs=«0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«LPCOAuthorizedParty»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:LPCOAuthorizedPartyNameTextType»/>
<xs:element name=«ID» type=«ds:LPCOAuthorizedPartyldentificationlDType» minOccurs=«0»7>
<xs:element name=«RoleCode» type=«ds:LPCOAuthorizcdPartyRolcCodcType»/>
<xs:element name=«Address»>
<xs:complexType>
<xs:sequence>
<xs:element name=«TypeCode» type- «ds:AddressTypeCodeType» minOccurs=«0»/>
<xs:element name=«CityName» type=«ds:AddressCityNameTextType» minOccurs=«0»/>
<xs:elcment name=«CountryCode» type-»ds:AddressCountryCodeType»/>
<xs:element name=«CountrySubDivisionCode»
type- «ds:AddressCountrySubDivisionCodeType» minOccurs=«0»/>
<xs:element name=«CountrySubDivisionName»
type- «ds:AddressCountrySubDivisionNameTextType» minOccurs=«0»/>
<xs:element name=«Line» typc=«ds:AddressLineTextType» minOccurs=«0»/>
<xs:element name^»TostcodelD» type=«ds:AddressPostcodeIDType» minOccurs=«0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«AdditionalInfoiTnation»>
<xs:complexType>
<xs:sequence>
<xs:element namc=«StatementCode» type=«ds:AdditionalInformationStatementCodcType»
minOccurs=«0»/>
<xs:element name=«StatementDescription»
type=«ds:AdditionalInformationStatementDescriptionTextType» minOccurs=«0»/>
<xs:element name- «LimitDateTime» type=«ds:AdditionalInformationLimitDatcTimeType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«GoodsShipment»>
<xs:complexType>
<xs:sequence>
<xs:element name=«ExportationCountryCode»
type=«ds:GoodsShipmcntExportationCountryCodeType»/>
<xs:element name=«AdditionalInformation» minOccurs=«0» maxOccurs=«unboundedM>
<xs:complexType>
<xs:sequence>
<xs:element name=«Content» type=«ds:AdditionalInfomiationContentTextType»/>
<xs:element name=«StatementCode» type=«ds:AdditionalInformationStatementCodeType»/>
<xs:element name=«StatementDescription»
type- «ds:AdditionalInformationStatementDescriplionTextType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Consignee» minOccurs=«0»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:ConsigneeNameTextType»/>
<xs:element name=«ID» type=«ds:ConsigneeIdentificationIDType» minOccurs=«0»/>
<xs:element name=«RoleCode» type=«ds:ConsigneeRoleCodeType»/>
<xs:element name=«Address»>
<xs:complexType>
<xs:sequence>
<xs:element name=«TypeCode» type=«ds:AddressTypeCodeType» minOccurs=:»0»/>
<xs:element name=«CityName» type=«ds:AddressCityNameTextType» minOccurs=«0»/>
<xs:element name=«CountryCode» type=«ds:AddressCountryCodeType»/>
<xs:element name- «CountrySubDivisionCode»
type=«ds:AddressCountrySubDivisionCodeType» minOceurs=«0»/>
<xs:element name=«CountrySubDivisionName»
type=«ds:AddressCountrySubDivisionNameTextType» minOccurs=«0»/>
<xs:element name=«Line» type=«ds:AddrcssLineTextType» minOccurs=«0»/>
<xs:element name- «PostcodelD»1 type=«ds:AddressPostcodelDType» minOccurs=«0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Contact» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:ContactNameTextType» minOccurs=«0»/>
<xs:element name=«Communication» minOccurs- «0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«ID» typc=«ds:CommunicationIdentificationIDType»/>
<xs:elemcnt name=«TypeID» type=«ds:CommunicationTypcIDType» minOccurs- «0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Communication» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«ID» type=«ds:CommunicationIdentificationIDType»/>
<xs:elementname- «TypelD» type=«ds:CommunicationTypeIDType» minOccurs=«0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Consignment» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«BorderTransportMeans» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name- «Name» type=«ds:BorderTransportMeansNameTextType» minOccurs=«0»/>
<xs:element пате=«Ш» type=«ds:BorderTransportMeansIdentificationIDType»
minOccurs=«0»/>
<xs:element name=«TypeCode» type=«ds:BorderTransportMeansTypeCodeType»/>
</xs:sequence>
</xs:complexType>
</xs:elements
<xs:element name=«LoadingLocation» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:LoadingLocationNameTextType»/>
<xs:element пате=«Ш» type=«ds:LoadingLocationIdentificationTDType»/>
<xs:element name=«DepartureDateTime» type=«ds:LoadingLocationDepartureDateTimeType»
minOccurs=«0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:elemcnt name=«UnloadingLocation» minOccurs- «0» maxOccurs=«unbounded»>
<xsxomplexType>
<xs:sequence>
<xs:element name=«ID» type=«ds:UnloadingLocationIdentificationIDType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name- «DeliveryDestination»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Address»>
<xs:complexType>
<xs:scquence>
<xs:element name=«CountryCode» type=«ds:AddressCountryCodeType»/>
</xs:sequence>
</xs:complexType>
</xs:clement>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Exporter»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:ExporterNameTextTypc»/>
<xs:element name-»ID» type=«ds:ExporterIdentificationIDType» minOccurs=«0»/>
<xs:element name=«RoIeCode» type=«ds:ExporterRoleCodeType»/>
<xs:element name- «Address»>
<xs:complexType>
<xs:sequence>
<xs:element name=«TypeCode» type=«ds:AddressTypcCodeType» minOccurs=«0»/>
<xs:element name=«CityName» type=«ds:AddressCityNameTextType» minOccurs=«0»/>
<xs:element name=«CountryCode» type=«ds:AddressCountryCodeType»/>
<xs:element name=«CountrySubDivisionCode»
type=«ds:AddressCountrySubDivisionCodeType» minOccurs=«0»/>
<xs:element name- «CountrySubDivisionName»
type=«ds:AddressCountrySubDivisionNameTextType» minOccurs=«0»/>
<xs:element name=«Line» type=«ds:AddressLineTextType» minOccurs=«0»/>
<xs:element name=«PostcodeID» type=«ds:AddressPostcodeIDType» minOccurs=«0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«GovemmentAgencyGoodsItem» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«SequenceNumeric» type=«ds:CommoditySequenceNumericType»/>
<xs:element name=«Commodity»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Description» type=«ds:Commodi) yDescriptionTextType»/>
<xs:elementname- «CountQuantity» type=«ds:CommodityCountQuantityType»
minOccurs=«0»/>
<xs:element name=«AdditionalInformation» minOccurs=«0»>
<xs:complexType>
<xs:sequence>
<xs:element name=«StatementCode» type- «ds:AdditionalInformationStatementCodeType»/>
<xs:element name=«StatementDescription»
type=«ds:AdditionalInformationStatementDescriptionTextType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:clement name=«Classification»>
<xs:complexType>
<xs:sequence>
<xs:element namc=«ID» type=«ds:ClassificationIdentificationIDType»/>
<xs:element name=«IdentificationTypeCode»
type=«ds:ClassificationIdentificationTypeCodeType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«GoodsMeasure» minOccurs=«0»>
<xs:complexType>
<xs:sequence>
<xs:element name=«GrossMassMeasure» type=«ds:GoodsMeasureGrossMassMeasureType»/>
<xs:element name=«NetNetWeightMeasure»
type «ds:GoodsMeasureNetNetWeightMeasureType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«ProductName» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:ProductNameNameTextType»/>
<xs:element name=«NameQualifierCode» type=«ds:ProductNameNameQualifierCodeType»
minOccurs=«0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Origin»>
<xs:complexType>
<xs:sequence>
<xs:element name=«RuleCodc» type=«ds:OriginRuleCodeType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name-»Packaging» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«MarksNumbersID» type=«ds:PackagingMarksNumbersIDType»
minOccurs=«0»/>
<xs:element name- «QuantityQuantity» type=«ds:PackagingQuantityQuantityType»/>
<xs:element name=«TypeCode» type=«ds:PackagingTypeCodeType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Importer»>
<xs:ccmplexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:ImporterNamcTextType»/>
<xs:element name=«ID» type=«ds:ExporterIdentificationIDType» minOccurs=«0»/>
<xs:element name- «RoleCode» type=«ds:ImporterRolcCodeType»/>
<xs:element name=«Address»>
<xs:complexType>
<xs:sequence>
<xs:element name=«TypeCode» type=«ds:AddressTypeCodeType» minOccurs=«0»/>
<xs:element name=«CityName» type=«ds:AddressCityNameTextType» minOccurs=«0»/>
<xs:element name- «CountryCode» type=«ds:AddressCountryCodeTypе»/>
<xs:element name=«CountrySubDivisionCode»
type- «ds:AddressCountrySubDivisionCodeType» minOccurs=«0»/>
<xs:element name- «CountrySubDivisionName»
type=«ds:AddressCountrySubDivisionNameTextType» minOccurs- «0»/>
<xs:element name=«Line» type- «ds:AddressLineTextType» minOccurs=«0»/>
<xs:element name=«PostcodeID» type=«ds:AddressPostcodeIDType» minOccurs- «0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Invoice» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«ID» type=«ds:InvoiceIdentificationIDType»/>
<xs:element name=«IssueDateTime» type- «ds:InvoiceIssueDateTimeType»/>
<xs:element name=«TypeCode» type=«ds:InvoiceTypeCodeType»/>
<xs:element name- «SequcnceNumeric» type=«ds:InvoiceSequenceNumericType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name- «PreviousDocumcnt» minOccurs- «0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«ID» type=«ds:PreviousDocumentIdentificationIDType»/>
<xs:element name=«IssueDateTime» type=«ds:PreviousDocumentIssueDateTimeType»/>
<xs:element name=«TypeCode» type-»ds:PreviousDocumentTypeCodeType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:schema>

Table C2
The scheme of electronic document data (information)
«Notification on absence of information» (Response)
<?xml version- «1.0» encoding=«UTF-8»?>
<xs:schema xmlns:xs=«http://www.w3.org/2001/XMLSchema«
xmlns=«um:wco:datamodel:WCO:Declaration:3» xmlns:ds- «urn:wco:datamodel:WCO:DS: l»
targetNamespace=«um:wco:datamodcl:WCO:Declaration:3»>
<xs:import namespace=«um:wco:datamodel:WCO:DS:l» schemaLocation=«DS_ lp0.xsd»/>
<xs:complexType name=«RootDocumentType»>
<xs:sequence>
<xs:element name=«FunctionalReferenceID»
typc=«ds:RootDocumentFunctionalReferenceIDType»/>
<xs:elemcnt name=«IssueDateTime» type=«ds:RootDocumentIssueDateTimeType»
minOccurs=«0»/>
<xs:element name=«AdditionalInformation» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name- «StatementDescription»
type=«ds:AdditionalInformationStatementDescriptionTextType»/>
</xs:sequence>
</xs:complexType>
</xs:elements
<xs:element name=«ContactOffice» minOccurs=«0»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Contact» minOccurs=«0» maxOccurs- «unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«Name» type=«ds:ContactNameTextType»/>
<xs:element name=«Communication» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element пате=«Ш» type=«ds:CommunicationIdentificationIDType»/>
<xs:element name=«TypeID» type=«ds:CommunicationTypeIDType» minOccurs=«0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Communication» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name- «ID» type=«ds:CommimicationIdentificationIDType»/>
<xs:element name=«TypeID» type=«ds:CommunicationTypeIDType» minOccurs-»0»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</xs:sequence>
</xs:complexType>
</xs:element>
<xs:elcmcnt name=«Error» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name- «ValidationCode» type=«ds:ErrorValidationCodeType»/>
<xs:element name=«Pointer» minOccurs=«0» maxOccurs=«unbounded»>
<xs:complexType>
<xs:sequence>
<xs:element name=«SequenceNumeric» type=«ds:PointerSequenceNumericType»/>
<xs:element name=«DocumentSectionCode» type=«ds:PointerDocumentSectionCodeType»/>
</xs:sequence>
</xs:complexType>
</xs:element>
</»xs:sequence>
</xs:complexType>
</xs:element>
<xs:element name=«Status»>

Table C3
The scheme of electronic document data (information)
«Request for information about certificates of origin» (Request)

<?xml version-11.0» encoding=«UTF-8»?>
<xs:schema xmlns:xs=«http://www.w3.org/2001/XMLSchema«
xmlns=«um:wco:datamodel:WCO:Declaration:1» xmlns:ds=«um:wco:datamodel:WCO:DS:1»
targetNamespace=«urn:wco:datamodel:WCO:Declaration:1»>
<xs:import namespace=«um:wco:datamodel:WCO:DS:l» schemaLocation=«DS_ lp0.xsd»/>
<xs:clement name=«RootDocument» type=«RootDocumentType»/>
<xs:complexType name=«RootDocumentType»>
<xs:sequence>
<xs:element name=«ID» type=«ds:RootDocumentIdentificationIDType» minOccurs=«0»/>
<xs:element name=«IssueDateTime» type=«ds:RootDocumentIssueDateTimeType»/>
<xs:element name=«issueLocationID»
type=«ds:RootDocumentIssueLocationIdentificationIDType» minOccurs- «0»/>
<xs:element name=«TypeCode» type=«ds:RootDocumentTypeCodeType»/>
</xs:sequence>
</xs:complexType>
</xs:schema>
Table C4
The scheme of acknowledgment and exception signals data

<?xmlversion=«1.0» encoding=«UTF-8»?>
<!--
Structure and requisite composition of acknowledgment and exception signals
  -->
<xs:schemaxmlns:xs=«http://www.w3.org/2001/XMLSchema« xmlns:sgn=«urn:EEC:signal:vl .0»  targetNamespace=«urn:EEC:signal:v1.0» elementFormDefault=«qualified»
attributeFormDefault=«unqualified»>
<xs:simplcType name=«EDoc!dType»>
<xs:annotation>
<xs:documentation>Document ID</xs:documentation>
</xs:annotation>
<xs:restriction base=«xs:token»>
 <xs: pattern value=«[0-9a-fA-F]{8}-[0-9a-fA-F]{4}-[0-9a-fA-F]{4}-[0-9a-fA-F]{4}-[0-9a-fA-
F]{ 12}»/>
</xs:restriction>
</xs:simpleType>
<xs:simpleType name=«DateTimeType»>
<xs:annotation>
<xs:documentation>Date by the Gregorian calendar and time in the Standard ISO 8601
format</xs:documentation>
</xs:annotation>
<xs:restriction base=«xs:dateTime»/> 
</xs:simpleType>
<xs:simpleType name=«ErrorCodeType»>
<xs:annotation>
<xs:documentation> Error code designation </xs:documentation>
</xs:annotation>
<xs:restriction base=«xs:token»>
<xs:minLength value=« l» />
<xs:maxLength vaIue=«255»/>
</xs:restriction>
</xs:simpleType>
<xs:simpleType name=«StringType»>
<xs:annotation>
<xs:documentation> Arbitrary information in text form </xs:documentation>
</xs:annotation>
<xs:restriction base=«xs:string»/>
</xs:simpleType>
<xs:complexType name=«DeliveryReceiptType»>
<xs:annotation>
<xs:documentation»«Receipt» confirmation signal Type </xs:documentation>
</xs:annotation>
<xs:sequence>
<xs:element name=«SignalId» type=«sgn:EDocIdType»/>
<xs:element name=«DateTime» type=«sgn:DateTimeType»/>
</xs:sequence>
</xs:complexType>
<xs:element name=«DeliveryReceipt» type=«sgn:DeliveryReceiptType»>
<xs:annotation>
<xs:documentation>«Receipt» confirmation signal </xs:documentation>
</xs:aimotation>
</xs:element>
<xs:complexType name=«ProcessingReceiptType»>
<xs:annotation>
<xs:documentation>«Processing Receipt» confinnation signal Type </xs:documentation>
</xs:annotation>
<xs:sequence>
<xs:element name=«SignalId» type=«sgn:EDocIdType»/>
<xs:element name=«Date Time» type=«sgn:DateTimeType»/>
</xs:sequence>
</xs:complexType>
<xs:element name=«ProcessingReceipt» type=«sgn:ProcessingReceiptType»>
<xs:annotation>
<xs:documentation>«Processing Receipt» confirmation signal </xs:documentation>
</xs:annotation>
</xs:element>
<xs:complexType name=«ValidationErrorType>>>
<xs:annotation>
<xs:documentation>«Error» Signal-exception Type </xs:documentation>
</xs:annotation>
<xs:sequence>
<xs:element name=«SignalId» type=«sgn:EDocIdType»>
<xs:annotation>
<xs:documentation> Signal-exception ID </xs:documentation>
</xs:annotation>
</xs:element>
<xs:element name=«DateTime» type=«sgn:DateTimeType»>
<xs:annotation>
<xs:documentation> Date and Time </xs:documentation>
</xs:annotation>
</xs:element>
<xs:element name=«Error» type=«sgn:ErrorType» maxOccurs=«unbounded»>
<xs:annotation>
<xs:documentation> Error Details </xs:documentation>
</xs:annotation>
</xs:element>
</xs:sequence>
</xs:comp1exType>
<xs:complexType name=«ErrorType»>
<xs:annotation>
<xs:documentation> Error Type </xs:documentation>
</xs:annotation>
<xs:sequence>
<xs:element name=«Code» type=«sgn:ErrorCodeType»>
<xs:annotation>
<xs:documentation> Control Error Code Designation </xs:documentation>
</xs:annotation>
</xs:element>
<xs:element name=«Description» type=«sgn:StringType»>
<xs:annotation>
<xs:documcntation> Control Error Code Designation </xs:documentation>
</xs:annotation>
</xs:element>
<xs:element name=«Details» type=«sgn:StringType» minOccurs=«0»>
<xs:annotation>
<xs:documentation> Error Detailed Information </xs:documentation>
</xs:annotation>
</xs:element>
<xs:element name=«EDocId» type=«sgn:EDocIdType» minOccurs=«0»>
<xs:annotation>
<xs:documentation> Identifier of the document in which the error occurred </xs:documentation>
</xs:annotation>
</xs:element>
<xs:element name=«Reference» type=«sgn:StringType» minOccurs=«0»>
<xs:annotation>
<xs:documentation> String of characters that makes it possible to locate unambiguously an element
in the document that caused an error </xs:documentation>
</xs:annotation>
</xs:element>
</xs:sequence>
</xs:complexType>
<xs:element name=«ValidationError» type=«sgn:ValidationErrorType»>
<xs:annotation>
<xs:documenlation>«ControlError» Signal-exception </xs:documentation>
</xs:aimotation>
</xs:element>
</xs:schema>


Appendix D. Examples of electronic documents
Table D1
Example of electronic message «Information on the issued certificate of origin» (ESS.VN.MSG.001)
<soap:Envelope xmlns:soap=«http://www.w3.org/2003/05/soap-envelope«
xmlns:urn=«um:EEC:Interaction:vl.O» xmlns:wsa=«http://www.w3.org/2005/08/addressing«>
<soap:Header>
<wsa:To>ESS.VN.VN</wsa:To>
<wsa:From>
<wsa:Address>E8S.VN.RU</wsa:Address>
</wsa:From>
<wsa:Action>tr://CERTIFICATE/0.1/ESS.VN.PRC.001/ESS.VN.TRN.001/ESS.VN.MSG.001</
wsa:Action>
<wsa:MessageID>um:uuid:dba8fff6-bbb3-47c3-afb2-a9a9accce8dd</wsa:MessageID>
</soap:Header>
<soap:Body>
<nl:RootDocument xsi:schemaLocation=«um:wco:datamodel:WCO:Declaration:2 Certificate.xsd» xmIns:xsi=«http://www.w3.org/2001/XMLSchema-instance« xmlns:nl=«um:wco:datamodel:WCO:Declaration:2»>
<CancellationDateTime>2017-12-17T00:00:00Z</CancellationDateTime>
<EffectiveDateTime>2017-10-15T00:00:00Z</EffectiveDateTime>
<ExpirationDateTime>2018-09-17T00:00:00Z</ExpirationDateTime>
<FunctionCode>CHG</FunctionCode>
<FunctionalReferenceID>PcaFAG0kNUGqHYoSTryWbg%3d%3d</FunctionalReferenceID>
<Ш>12345</ID>
<IssueDateTime>2017-09-17T09:30:00Z</IssueDateTime>
<issueLocationID>RU MOW</issueLocationID>
<TypeCode>EAV</TypeCode>
<AdditionalDocument>
<IssueDateTime>2017-09-17T00:00:00Z</IssueDateTime>
<issueLocationID>RUMOW</issueLocationID>
<IssueLocationName>Russian Federation, Moscow</IssueLocationName>
<Authenticator>
<Name>The Chamber of Commerce and Industry of the Russian Federation (CCI of Russia)</Name>
<ID>1027746000853</ID>
<RoleCode>AX</RoleCode>
<Address>
<TypeCode>2</TypeCode>
<CityName>Moscow</CityName>
<CountryCode>RU</CountryCode>
<Line>llyinka 6/1, 1 Moscow, Russian Federation</Line>
<PostcodeID>109012</Postcodero>
</Address>
</Authenticator>
<LPCOAuthorizedParty>
<Name>RostovVinTrade</Name>
<ID>1234567890987</ID>
<RoleCode>DT</RoleCode>
<Address>
<TypeCode>2</TypeCodc>
<CityName>Rostov-on-Don</CityName>
<CountryCode>RU</CountryCode>
<Line>Rostov-on-Don, Lenina st, 18, Russia</Line>
<PostcodeID>344012</PostcodeID>
</Address>
</LPCOAuthorizedParty>
</AdditionalDocument>
<AdditionalInformation>
<StatementCode>R.TR</StatementCode>
<StatementDescription>Issued Retroactively</StatementDescription>
<LimitDateTime>2017-09-16T00:00:00Z</LimitDateTime>
</AdditionalInformation>
<GoodsShipment>
<ExportationCountryCode>RU</ExportationCountryCode>
<AdditionalInformation>
<Content>Invoice will be issued later by Asia Grocery Distribution Limited. Address : 4/F How
Ming Factory Building, 99 How Ming Street, Kwun Tong</Content>
<StatementCode>TCI</StatementCode>
<StatementDescription>Third Country Invoice</StatementDescription>
</AdditionalInformation>
<Consignee>
<Name>LEE KHOA TRADING</Name>
<RoleCode>CN</RoleCode>
<Address>
<CityName>Hanoi</CityName>
<CountryCode>VN</CountryCode>
<Line>Add. 44/4 Dang Van Ngu Str., Dong Da Distr.,Hanoi, Viet Nam, 115000 </Line>
</Address>
</Consignee>
<Consignment>
<BorderTransportMeans>
<TypeCode listAgencyName=«EAEU»>40</TypeCode>
</BorderTransportMeans>
<LoadingLocation>
<Name>Russiian Federation, Moscow</Name>
<ID>RUSVO</ID>
</LoadingLocation>
<UnloadingLocation>
<ID>VNHAN</ID>
</UnloadingLocation>
</Consignment>
<DeliveryDestination>
<Address>
<CountryCode>VN</CountryCode>
</Address>
</DeliveryDestination>
<Exporter>
<Name>RostovVinTrade</Name>
<RoleCode>EX</RoleCode>
<Address>
<TypeCode>2 </TypeCode>
<CityName>Rostov-on-Don</CityName>
<CountryCode>RU</CountryCode>
<Line>Rostov-on-Don, Lenina st, 18, Russia, 344012</Line>
</Address>
</Exporter>
<GovernmentAgencyGoodsItem>
<SequenceNumeric>1</SequenceNumeric>
<Commodity>
<Description>Sparkling wine</Description>
<CountQuantity unitCode=«796»>144</CountQuantity>
<Classification>
<ID>2204101100</ID>
<IdentificationTypeCode>HS code</IdentificationTypeCode>
</Classification>
<GoodsMeasure>
<GrossMassMeasure unitCode=«166»>80</GrossMassMeasure>
<NetNetWeightMeasure unitCode=«166»>60</NetNetWeightMeasure>
</GoodsMeasure>
<ProductName>
<Name>Rostovskoye Igristoye</Name>
<NameQualifierCode>brand name</NameQualifierCode>
</ProductName>
</Commodity>
<Origin>
<RuleCode>WO</RuleCode>
</Origin>
<Packaging>
<QuantityQuantity>1</QuantityQuantity>
<TypeCode>32</TypeCode>
</Packaging>
</GovernmentAgencyGoodsItem>
<GovernmentAgencyGoodsItem>
<SequenceNumeric>2</SequenceNumeric>
<Commodity>
<Description>Dry white wine</Description>
<CountQuantity unitCode=«796»>144</CountQuantity>
<Ciassification>
<ID>2204210700</Ш>
<IdentificationTypeCode>HS code</IdentificationTypeCode>
</Classification>
<GoodsMeasure>
<GrossMassMeasure unitCode=«166»>70</GrossMassMeasure>
<NetNetWeightMeasure unitCode=«166»>55</NetNetWeightMeasure>
</GoodsMeasure>
<ProductName>
<Name>TSIMLYANSKY RESERVE</Name>
<NameQualifierCode>brand name</NameQualifierCode>
</ProductName>
</Commodity>
<Origin>
<RuleCode>W0</RuleCode>
</Origin>
<Packaging>
<QuantityQuantity> l</QuantityQuantity>
<TypeCode>32</TypeCode>
</Packaging>
</GovemmentAgencyGoodsItem>
<GovemmentAgencyGoodsItem>
<SequenceNumeric>3</SequenceNumeric>
<Commodity>
<Description>vodka</Description>
<CountQuantity unitCode=«796»> l 44</CountQuantity>
<Classification>
<ID>2208601100</ID>
<IdcntificationTypeCode>HS code</IdentificationTypeCode>
</Classification>
<GoodsMeasure>
<GrossMassMeasure unitCode=«166»>60</GrossMassMeasure>
<NetNetWeightMeasure unitCode=«166»>50</NetNetWeightMeasure>
</GoodsMeasure>
<ProductName>
<Name>Ataman Platov</Name>
<NamcQualifierCode>brand name</NameQualifierCode>
</ProductName>
</Commodity>
<Origin>
<RuleCode>WO</RulcCode>
</Origin>
<Packaging>
<QuantityQuantity> l</QuantityQuantity>
<TypeCode>32</TypeCode>
</Packaging>
</GoveramentAgencyGoodsItem>
<Importer>
<Name>LEE KHOA TRADING</Name>
<RoleCode>CN</RoleCode>
<Address>
<TypeCode>2</TypeCode>
<CityName>Hanoi</CityName>
<CountryCode>VN</CountryCode>
<Line>Add. 44/4 Dang Van Ngu Sir., Dong Da Distr.,Hanoi, Viet Nam, 115000 </Line>
</Address>
</Importer>
<Invoice>
<ID>12345</ID>
<IssueDateTime>2017-08-17T00:00:00Z</IssueDateTime>
<TypeCode>02017</TypeCode>
<SequenceNumeric>1</SequenceNumeric>
</Invoice>
<Invoice>
<ID>12333</1D>
<IssucDateTime>2017-08-17T00:00:00Z</IssueDateTime>
<TypeCode>02017</TypeCode>
<SequenceNumeric>1</SequenceNumeric>
</Invoice>
<Invoice>
<ID>12444</ID>
<IssueDateTime>2017-08-18T00:00:00Z</IssueDateTime>
<TypeCode>02017</TypeCode>
<SequenceNumeric>2</ScquenceNumcric>
</Invoice>
<Invoice>
<ID>12555</ID>
<IssueDateTime>2017-08-19T00:00:00Z</IssueDateTime>
<TypeCode>02017</TypeCode>
<SequenceNumeric>3</SequenceNuraeric>
</Invoice>
</GoodsShipment>
<PreviousDocument>
<ID>12097</ID>
<IssueDateTime>2017-09-01TOO:00:OOZ</IssueDateTime>
<TypeCode>861</TypeCode>
</PreviousDocument>
</nl:RootDocument>
</soap:Body>
</soap:Envelope>

Table D2
Example of electronic message «Notice on the results of processing of information» (ESS.VN.MSG.002)
<scap:Envelope xmlns:soap=«http://www.w3.org/2003/05/soap-envelope« xmlns:urn=«um:EEC:Interaction:vl.O» xmlns:wsa- «http://www.w3.org/2005/08/addressing«>
<soap:Header>
<wsa:To>ESS.VN.VN</wsa:To>
<wsa:From>
<wsa:Address>ESS.VN.RU</wsa:Address>
</wsa:From>
<wsa:Action>tr://CERTIFICATE/0.1/ESS.VN.PRC.001/ESS.VN.TRN.001/ESS.VN.MSG.002</
wsa:Action>
<wsa:MessageID>urn:uuid:55cc361 l -b3b4-4cfa-aebb-el 2c4a48d20e</wsa:MessagelD>
<wsa:RelatesTo>um:uuid:dba8fff6-bbb3-47c3-afb2-a9a9acccc8dd</wsa:RclatesTo>
</soap:Header>
<soap:Body>
<nl :RootDocumcnt xsi:schemaLocation=«urn:wco:datamodel:WCO:Declaration:3 Response.xsd» xmlns:xsi=«http://www.w3.org/2001/XMLSchema-instance« xmlns:nl=«urn:wco:datamodel:WCO:Declaration:3»>
<Additionalbiformation>
<StatementDescription>Success</StatemertDescription>
</AdditionalInformation>
<Status>
<NameCode>0</NameCode>
<ReleaseDateTi me>2017-09-17T12:33:47Z</RcleaseDateTime>
</Status>
<Declaration>
<FunctionalReferenceID>f6819dcd-0df4-40e2-9c9b-40df4b3c0e4</FunctionalReferenceID>
<ID>12345</ID>
</Declaration>
</nl:RootDocument>
</soap:Body>
</soap:Envelope>

         Table D3
Example of electronic message «Notice on absence of information»
(ESS.VN.MSG.003)
<soap:Envelope xmlns:soap=«http://www.w3.org/2003/05/soap-envelope« xmlns:um=«um:EEC:Interaction:vl .O» xmlns:wsa=«http://www.w3.org/2005/08/addressing«>
<soap:Header>
<wsa:To>ESS.VN.VN</wsa:To>
<wsa:From>
<wsa:Address>ESS.VN.RU</wsa:Address>
</wsa:From>
<wsa:Action>tr://CERTIFICATE/0.1/ESS.VN.PRC.002/P.EE.02.TRN.002/ESS.VN.MSG.003</
wsa:Action>
<wsa:MessageID>um:uuid:55cc361 l -b3b4-4cfa-aebb-el 2c4a48d20e</wsa:MessageID>
<wsa:RelatesTo>urn:uuid:23ccf7cb-c507-404f-aa78-4ffll 52a6633a </wsa:RelatesTo>
</soap:Header>
<soap:Body>
<nl :RootDocument xsi:schemaLocation=«um:wco:datamodel:WCO:Declaration:3 Response.xsd» xmlns:xsi=«hltp://www.w3.org/2001/XMLSchema-instance« xmlns:nl=«um:wco:datamodel:WCO:Declaration:3»>
<AdditionalInformation>
<StatementDescription>Success</StatementDescription>
</AdditionalInformation>
<Status>
<NameCode> l </NameCode>
<ReleaseDateTime>2017-09-17T12:33:47Z</RelcaseDateTime>
</Status>
<Declaration>
<FunctionalReferenceID>f6819dcd-0df4-40e2-9e9b-40df4b3c0e4</FunctionalReferenceID>
<ID>12345</ID>
</Declaration>
</nl:RootDocument>
</soap:Body>
</soap:Envelope>


Table D4 
Example of electronic message «Request for information on the certificate of origin» (ESS.VN.MSG.004)
<soap:Envelope xmlns:soap=«http://www.w3.org/2003/05/soap-envelope« xmlns:um=«urn:EEC:Interaction:vl .O» xmlns:wsa=«http://www.w3.org/2005/08/addressing«>
<soap:Header>
<wsa:To>ESS.VN.RU</wsa:To>
<wsa:From>
<wsa:Address>ESS.VN.VN</wsa:Address>
</wsa:From>
<wsa:Action>tr://CERT1FICATE/O. l /ESS.VN.PRC.002/ESS.VN.TRN.002/ESS.VN.MSG.004</
wsa:Action>
<wsa:MessagcID>urn:uuid:23ccf7cb-c507-404f-aa78-4f0152a6633a</wsa:MessageID>
</soap:Header>
<soap:Body>
<nsl :RootDocument xsi:schemaLocation=«um:wco:datamodcl:WCO:Declaration: l Request.xsd» xmlns:xsi=«http://www.w3.org/2001/XMLSchema-instance« xmlns:nsl=«um:wco:datamodel:WCO:Dcclaration:l»>
<Ш>12345</ГО>
<IssueDateTime>2016-12-17T00:00:00Z</IssueDateTime>
<issueLocationlD>RUMOW</issueLocationID>
<TypeCode>EAV</TypeCode>
</ns1:RootDocumcnt>
</soap:Body>
</soap:Envelope>

Table D5
Example of electronic message «Information on the issued certificate of origin provided in response to the request» (ESS.VN.MSG.005)
<soap:Envelope xmlns:soap=«http://www.w3.org/2003/05/soap-envelope«
xmlns:um=«urn:EEC:Interaction:vl.O» xmlns:wsa=«http://www.w3.org/2005/08/addressing«>
<soap:Header>
<wsa:To>ESS.VN.VN</wsa:To>
<wsa:From>
<wsa:Address>ESS.VN.RU</wsa:Address>
</wsa:From>
<wsa:Action>tr://CERTIFICATE/0.1/ESS.VN.PRC.002/ESS.VN.TRN.002/ESS.VN.MSG.005</
wsa:Action>
<wsa:MessageID>um:uuid:84cec07f-122f-459e-a5ef-70718845269 l </wsa:MessagelD>
<wsa:RelatesTo>um:uuid:23ccf7cb-c507-404f-aa78-4f0152a6633a</wsa:RelatesTo>
</soap:Header>
<soap:Body>
<nl:RootDocument xsi:schemaLocation=«um:wco:datamodel:WCO:Declaration:2 Certificate.xsd» xmlns:xsi=«http://www.w3.org/2001/XMLSchema-instance« xmlns:nl=«um:wco:datamodel:WCO:Declaration:2»>
<CancellationDateTime>2017-12-17T00:00:00Z</CancellationDateTime>
<EffectiveDateTime>2017-10-15T00:00:00Z</EffectiveDateTime>
<ExpirationDateTime>2018-09-17T00:00:00Z</ExpirationDateTime>
<FunctionCode>CHG</FunctionCode>
<FunctionaIReferenceID>PcaFAG0kNUGqHYoSTryWbg%3d%3d</FunctionalReferenceID>
<ID>12345</ID>
<IssueDatcTime>2017-09-17T09:30:00Z</IssueDateTirae>
<issueLocationID>RUMOW</issueLocationID>
<TypeCode>EAV</TypeCode>
<AdditionalDocument>
<IssueDateTime>2017-09-17T00:00:00Z</IssueDateTime>
<issueLocationID>RUMOW</issueLocationID>
<IssueLocationName>Russian Federation, Moscow</IssueLocationName>
<Authenticator>
<Name>The Chamber of Commerce and Industry of the Russian Federation (CCI of Russia)</Name>
<ID>1027746000853</ID>
<RoleCode>AX</RoleCodc>
<Address>
<TypeCode>2</TypeCode>
<CityName>Moscow</CityName>
<CountryCode>RU</CountryCode>
<Line>llyinka 6/1, 1 Moscow, Russian Federation</Line>
<PostcodeID>109012</PostcodeID>
</Address>
</Authenticator>
<LPCOAuthorizedParty>
<Name>RostovVinTrade</Name>
<ID>1234567890987</ID>
<RoleCode>DT</RoleCode>
<Address>
<TypeCode>2</TypeCode>
<CityName>Rostov-on-Don</CityName>
<CountryCode>RU</CountryCode>
<Line>Rostov-on-Don, Lenina st, 18, Russia</Line>
<PostcodeID>344012</PostcodeID>
</Address>
</LPCOAuthorizedParty>
</AdditionalDocumcnt>
<AdditionalInformation>
<StatementCode>R.TR</StatementCode>
<StatementDescription>Issued Retroactively</StatementDescription>
<LimitDateTime>2017-09-16T00:00:00Z</LimitDateTime>
</AdditionalInformation>
<GoodsShipment>
<ExportationCountryCode>RU</ExportationCountryCode>
<AdditionalInformation>
<Content>Invoice will be issued later by Asia Grocery Distribution Limited. Address : 4/F How
Ming Factory Building, 99 How Ming Street, Kwun Tong</Content>
<StatementCode>TCI</StatementCode>
<StatementDescription>Third Country Invoice</StatementDescription>
</AdditionalInformation>
<Consignee>
<Name>LEE KHOA TRADING</Name>
<RoleCode>CN</RoleCode>
<Address>
<CityName>Hanoi</CityName>
<CountryCode>VN</CountryCode>
<Line>Add. 44/4 Dang Van Ngu Str., Dong Da Distr.,Hanoi, Viet Nam, 115000 </Line>
</Address>
</Consignee>
<Consignment>
<BorderTransport Means>
<TypeCode HstAgencyName=«EAEU»>40</TypeCode>
</BorderTransportMeans>
<LoadingLocation>
<Name>Russiian Federation, Moscow</Name>
<ID>RUSVO</ID>
</LoadingLocation>
<UnloadingLocation>
<ID>VNHAN</ID>
</UnloadingLocation>
</Consignment>
<DeliveryDestination>
<Address>
<CountryCode>VN</CountryCode>
</Address>
</DeliveryDestination>
<Exporter>
<Name>RostovVinTrade</Name>
<RoleCode>EX</RoleCode>
<Address>
<TypeCode>2</TypeCode>
<CityName>Rostov-on-Don</CityName>
<CountryCode>RU</CountryCode>
<Line>Rostov-on-Don, Lenina st, 18, Russia, 344012</Line>
</Address>
</Exporter>
<GovemmentAgencyGoodsItem>
<SequenceNumeric>1</SequenceNumeriO
<Commodity>
<Description>Sparkling wine</Description>
<CountQuantity unitCode=«796»>144</CounlQuantity>
<Classification>
<ГО>2204101100</Ш>
<IdentificationTypeCode>HS code</IdentificationTypeCode>
</Classification>
<GoodsMeasure>
<GrossMassMeasure unitCode=«166»>80</GrossMassMeasure>
<NetNetWeightMeasure unitCode=«166»>60</NetNetWeightMeasure>
</GoodsMeasure>
<ProductName>
<Name>Rostovskoye Igristoye</Name>
<NameQualifierCode>brand name</NameQualifierCode>
</ProductName>
</Commodity>
<Origin>
<RuleCode>WO</RuleCode>
</Origin>
<Packaging>
<QuantityQuantity> l </QuantityQuantity>
<TypeCode>32</TypeCode>
</Packaging>
</GovernmentAgencyGoodsItem>
<GovemmentAgencyGoodsItem>
<SequenceNumeric>2</SequenceNumeric>
<Commodity>
<Description>Dry white wine</Description>
<CountQuantity unitCode=«796»>144</CountQuantity>
<Classification>
<ID>2204210700</ID>
<IdentificationTypeCode>HS code</IdentificationTypcCode>
</Classification>
<GoodsMeasurc>
<GrossMassMeasure unitCode-»166»>70</GrossMassMeasure>
<NetNetWeightMeasure unitCode=«166»>55</NetNetWeightMeasure>
</GoodsMeasure>
<ProductName>
<Name>TSIMLYANSKY RESERVE</Name>
<NameQualifierCode>brand name</NameQualifierCode>
</ProductName>
</Commodity>
<Origin>
<RuleCode>W0</RuleCode>
</Origin>
<Packaging>
<QuantityQuantity>1</QuantityQuantity>
<TypeCode>32</TypeCode>
</Packaging>
</GovemmentAgencyGoodsItem>
<GovernmentAgencyGoodsItcm>
<SequenceNumeric>3</SequenceNumeric>
<Commodity>
<Dcscription>vodka</Description>
<CountQuantity unitCodc=«796»>144</CountQuantity>
<Classification>
<Ш>2208601100</Ю>
<IdentificationTypeCode>HS code</IdentificationTypeCode>
</Classification>
<GoodsMeasure>
<GrossMassMeasure unitCode=«166»>60</GrossMassMeasure>
<NetNetWeightMeasure unitCode=«166»>50</NetNetWeightMeasure>
</GoodsMeasure>
<ProductName>
<Name>Ataman Platov</Name>
<NameQualifierCode>brand namc</NameQualifierCode>
</ProductName>
</Commodity>
<Origin>
<RuleCode>WO</RuleCode>
</Origin>
<Packaging>
<QuantityQuantity> l </QuantityQuantity>
<TypeCode>32</TypeCode>
</Packaging>
</GovemmcntAgencyGoodsItem>
<Importer>
<Name>LEE KHOA TRADING</Name>
<RoleCode>CN</RoleCode>
<Address>
<TypeCode>2</TypeCode>
<CityName>Hanoi</CityName>
<CountryCode>VN</CountryCode>
<Line>Add. 44/4 Dang Van Ngu Str., Dong Da Distr.,Hanoi, Viet Nam, 115000 </Line>
</Address>
</Importer>
<Invoice>
<ID>12345</ID>
<IssueDateTime>2017-08-17T00:00:00Z</IssueDateTime>
<TypeCode>02017</TypeCode>
<SequenceNumeric> l </SequenceNumeric>
</Invoice>
<Invoice>
<ID>12333</ID>
<IssueDateTime>2017-08-17T00:00:00Z</IssueDateTime>
<TypeCode>02017</TypeCode>
<SequenceNumeric>1</SequenceNumeric>
</Invoice>
<Invoice>
<Ш>12444</Ш>
<IssueDateTime>2017-08-18T00:00:00Z</IssueDateTime>
<TypeCode>02017</TypeCode>
<SequenceNumeric>2</SequenceNumeric>
</Invoice>
<Invoice>
<Ш>12555</Ш>
<IssueDateTime>2017-08-19T00:00:00Z</IssueDateTime>
<TypeCode>02017</TypeCode>
<SequenceNumeric>3</SequenceNumeric>
</Invoice>
</GoodsShipment>
<PreviousDocument>
<ID>12097</ID>
<IssueDateTime>2017-09-01T00:00:00Z</IssueDateTime>
<TypeCode>861</TypeCode>
</PreviousDocument>
</nl:RootDocument>
</soap:Body>
</soap:Envelope>


Appendix E. Directories and classifiers
Table El

Units of measurement Classifier (used in the Union)

	Code
	Name


	166
	Kilogram

	797
	Hundred pieces

	246
	1000 kilowatt hour

	130
	1000 liters

	114
	1000 cubic meters

	798
	Thousand pieces

	163
	Grams

	306
	Gram fissile isotopes

	162
	Metric carats ( lcarat=2*10 (-4) kg

	845
	Kilogram of dry (90% ) substance

	841
	Kilogram of hydrogen peroxide

	852
	Kilogram of potassium oxide

	859
	Kilogram of potassium hydroxide

	861
	Kilogram of nitrogen

	863
	Kilogram of sodium hydroxide

	865
	Kilogram of phosphorus pentoxide

	867
	Kilogram of uranium

	305
	Curie

	112
	Litre

	831
	Liter of pure (100%) alcohol

	006
	Meter

	055
	Square meter

	113
	Cubic meter

	715
	Pair

	185
	Capacity in tons

	796
	Piece



Units of measurement Classifier (used in the Viet Nam)


	Code
	Name

	DUNK
	10 units

	DPCE
	10 pieces

	DMTR	
	10 meters

	HPCE	
	100 pieces

	HFT	
	100 FT

	HGRM	
	100 GRAMME

	HMTR	
	100 meters

	HUNV	
	100 units

	KSET
	1000 sets

	KPCE
	1000 pieces

	KUNC
	1000 units

	KROL	
	1000 rolls

	KPR
	1000 pairs

	KPKG	
	1000 packs

	KUNK	
	1000 boxes

	KMTK	
	1000 square meters

	KPIP
	1000 pipes

	KUNQ
	1000 units

	КPRO	
	1000 products

	KUNV	
	1000 unit

	KMTQ	
	1000m2

	ONZ
	Ounce

	OII
	Ounce (including package)

	OIC
	Ounce (including container)

	OMC
	Ounce (by metal content)

	ODW
	Ounce (by dry weight)

	OZI
	Measurement Ounce

	BAN 
	Piece

	BANG
	Piece

	BBL
	Barrel

	BICH
	Piece

	SET
	Set

	PCE
	Piece

	UNH
	Unit

	CT
	Cara

	UNY 
	Unit 

	CEN
	Centimeter

	UNA
	Bottle

	CHI
	CHI

	СМ2	
	cm2

	СМ3
	cm3

	UNC
	unit

	CONT 
	CONTAINER

	UNU
	Piece

	CUC
	Unit

	CUM
	Group of unit

	UNN
	Roll

	ROL
	Roll

	DM
	dm

	DM2
	dm2

	PR
	pair

	GLL 
	Galon

	GRM	
	Gramme

	GII 
	Gramme (including package) 

	GIC
	Gramme (including container)

	GMC
	Gramme (by metal content)

	GDW
	Gramme (by dry weight)

	PKG
	Package

	LC	
	lactose contained

	HLTR
	Hectoliter

	YRD
	Yard

	YDQ
	Cubic yard

	YDK
	Square yard

	INC
	Inch

	UNK
	Pack/box

	KL
	Kiloliter

	KMTR
	Kilometer (1000 meters)

	KHW
	Kilowatt hour

	KGM
	Kilogram

	KII
	Kilogram (including package)

	KIC
	Kilogram (including container)

	KMC
	Kilogram (by metal content)

	KDW
	Kilogram (by dry weight)

	KIT
	KIT

	KVA
	KVA

	LIEU
	Dose

	LTR
	Litter

	QT
	British litter

	LOT
	Lot

	UNL
	can

	MTR
	meter

	MTQ
	cubic meter

	MTK
	square meter

	MGRM
	Milligrams

	MLT
	Milliliters

	MMTR
	Millimeter

	ММ2
	mm2

	ММ3
	mm3

	TH
	Thousands

	PIP
	Pipe

	PTI
	Pints

	LBR
	Pounds

	LII
	Pounds (including package)

	LIC
	Pounds (including container)

	LMC
	Pounds (by metal content)

	LDW
	Pounds (by dry weight)

	FOT
	Feet

	FTQ
	Cubic feet

	FTK
	Square feet

	UNQ
	Pieces

	UNB
	Quyen/Tap

	RAM
	RAM

	SOI
	String

	STER
	Ster

	DZN
	Dozens

	HKGM
	Quintal (100kg)

	TAM
	Piece

	TNE
	Ton

	MII
	Tons (including package)

	MIC
	Tons (including container)

	MMC
	Tons (by metal content)

	MDW
	Tons (by dry weight)

	LTN
	Long tons

	STN
	Short tons

	UNT
	Piece

	TO
	Sheet

	GRO
	Gross

	GT
	Gross tonnage

	TRO
	Troy ounce

	DPT
	Tonnage

	BAG
	Bag

	UND
	Unit

	UNV
	Unit

	UNIT
	UNIT

	LBS
	LBS

	VI
	

	INC2
	Grid

	Inch2
	

	SYS
	System

	PRO
	Product

	PAIL
	Barred



Table E2
Classifier of transport and transportation of goods (used in the Union)


	Code
	Name

	10
	Sea transport*

	20
	Railway transport*

	30
	Road transport*

	40
	Air transport*

	50
	Mailing

	71
	Pipeline transport

	72
	Power 

	80
	Inland waterway transport *

	90
	Vehicles transported as goods under their own power

	99
	Others



* Including any vehicle which is transported by said transport type.

Classifier of transport and transportation of goods (used in the Viet Nam)
	Code

	Name

	1
	Air route

	2
	Sea route (container)

	3
	Sea route (un-container)

	4
	Land route (truck)

	5
	Rail way

	6
	River route

	9
	Others




Table ЕЗ

Classifier of documents types used for customs declaration
(used in the Union)

	Code

	Name

	2, Transport (shipping) documents

	02011
	Bill of lading

	02012
	Waybill for the carriage of goods by water transport

	02013
	Railway invoice

	02024
	TIR carnet

	02025
	ATA camet

	02022
	Baggage check

	02014
	Other documents required by the rules of railway transportation

	02015
	Waybill under the Convention on the Contract for the International Carriage of Goods1956

	02016
	Another waybill for the carnage of goods by road transport

	02017
	Air waybill

	02018
	Transport documents used in the movement of goods through pipelines or power transmission lines

	02019
	Postal waybill

	02020
	General waybill for express delivery

	02021
	Individual waybill for express delivery

	02026
	Packing List

	02099
	Other transport (shipping) documents

	3. Documents confirming the consummation of foreign trade transaction or other documents
confirming the right of possession, use and (or) disposal of goods

	03011
	Agreement (contract), concluded when consummating the foreign trade transaction

	03012
	Documents ammending or supplementing the document, the details of which are listed under code 03011

	03013
	Document confirming consummation of unilateral foreign trade transaction

	03014
	Documents confirming the right of possession, use and (or) disposal of goods in the absence of any transaction

	03021
	Documents confirming the transfer of intellectual property rights (author, license

	03022
	Documents confirming the introduction into circulation of goods designated by the trademark within the customs territory of the Customs Union, with the consent of the

	03999
	Other documents confirming the right of possession, use and (or) disposal of goods

	4. Commercial documents

	04021
	Invoice to the Contract

	04022
	Other settlement or commercial documents (including cash or sales receipt for the purchase of goods in retail stores)

	04023
	Bank documents (if the invoice is paid, depending on the conditions of foreign trade contract), as well as other payment documents reflecting the value of the goods

	04025
	Pro forma invoice to the Contract

	04031
	Invoice for the carriage (transportation), loading, unloading and reloading goods

	04032
	Bank or other payment documents for payment of transportation costs, reflecting the cost of transportation (transportation), loading, unloading and reloading goods

	04033
	Contract on transportation, loading, unloading or reloading goods

	04041
	Invoices for provision of broking services

	04042
	Bank or other payment documents for provision of broking services

	04043
	Broking service agreement

	04051
	Documents on the value of goods and services provided to customers free of charge or
at reduced prices for use in connection with the production and sale

	04061
	Invoice containing information on payments for the use of intellectual property

	04062
	Bank payment documents, accounting and other documents containing information on
payments for the use of intellectual property

	04071
	Documents (including accounting) and information containing data on part of the income (revenue), which directly or indirectly is owed to the seller as a result of the subsequent sale, disposition or other means of use of goods

	04081
	Invoice that contains information about the cost of packaging materials and (or) work
on the packaging

	04082
	Bank or other payment documents on the cost of packaging materials and (or) work 
on the packaging

	04083
	Contract on the cost of cargo containers, packaging, packaging materials and works
on packaging

	04091
	Accounting records of producer of goods being valued, which contain information on the costs of production or acquisition of materials, of production costs, as well as other operations related to the production of imported goods, commercial invoices of producer of goods being valued, prepared in accordance with generally accepted accounting principles

	04101
	Invoice on the cost of design, development, engineering, artwork, drawings and
sketches

	04102
	Bank or other payment documents on the cost of design, development, engineering,
artwork, drawings and sketches

	04111
	Invoice for provision of insurance services

	04112
	Bank or other payment documents on the cost of insurance services

	04113
	Insurance policy

	04115
	Insurance contract

	04121
	Quotes of the world»s stock exchanges

	04999
	Other documents and information that the customs applicant can provide in support of
the declared customs value

	6. Documents confirming and (or) containing information about the country of origin

	06011
	The certificate of origin (form CT-1)

	06013
	The certificate of origin (form A)

	06014
	Non-preferential certificate of origin (general form)

	06015
	Advance ruling on the country of origin

	06016
	Declaration of origin

	06017
	The certificate of origin (form CT-2)

	06018
	The certificate of origin (form EAV)

	06999
	Other documents confirming the origin of goods



Classifier of documents types used for customs declaration
(used in Viet Nam)

	Code
	Name

	INV
	Invoice

	BOL 
	B/L (Bill of Lading)

	AWB
	AWB (Air Waybill)

	INS
	Details of insurance

	CON
	Contract

	ALL
	All application dossier

	ETC
	Other




Appendix F. The description of web-services

Table FI
Description of Web-services in WSDL-fonnat
<?xml version-»1.0» encoding=«utf-8»?>
<wsdl:definitions xmlns:tns=«http://tempuri.org/« xmlns:ls_ l =«um:wco:datamodel:WCO:Declaration: l» xmlns:ls_2=«urn:wco:datamodel:WCO:Declaration:2»
xmlns:Is_3=«um:wco:datamodel:WCO:Declaration:3» xmlns:sgn=«um:EEC:signal:vl.O» xmlns:wsdl=«http://schemas.xmlsoap.org/wsdl/« xmlns:wsam=«http://www.w3.org/2007/05/addressing/metadata«
xmlns:soapl 2=«http://schemas.xmlsoap.org/wsdl/soapl 2/» name=«EECVNCertificateService»
targetNamespace=«http://tempuri.org/«>
<wsdl:types>
<xsd:schema xmlns:xsd- «http://www.w3.org/2001/XMLSchcma« targetNamespace=«http://tempuri.org/« xmlns:ls_l=«um:wco:datamodel:WCO:Declaration: 1» xmlns:ls_2=«um:wco:datamodel:WCO:Declaration:2»
xmlns:ls_3=«um:wco:datamodcl:WCO:Declaration:3» xmlns:sgn=«um:EEC:signal:vl.O»
elementFormDefault=«qualified»>
<xsd:import namespace=«um:wco:datamodel:WCO:Declaration:l»
schemaLocation=«Request.xsd»/>
<xsd:import namespace=«um:wco:datamodel:WCO:Declaration:2»
schemaLocation=«Certificate.xsd»/>
<xsd:import namespace=«urn:wco:datamodel:WCO:Declaration:3»
schemaLocation=«Response.xsd»/>
<xsd:import namespace=«urn:EEC:signal:vl .0» schemaLocation=«EECSoapSignal.xsd»/>
<xsd:element name=«sendCertificateDetails»>
<xsd:complexType>
<xsd:sequence>
<xsd:element name=«RootDocument» type=«ls_2:RootDocumentType»/>
</xsd:sequence>
</xsd:complexType>
</xsd:element>
<xsd:element name- «sendRequestCertificateDetails»>
<xsd:complexType>
<xsd:sequence>
<xsd:element name=«RootDocument» type=«ls_l:RootDocumentType»/>
</xsd:sequence>
</xsd:complexType>
</xsd:element>
<xsd:elemcnt name=«sendResultCertificateDetails»>
<xsd:complexType>
<xsd:sequence>
<xsd:element name:=«RootDocument» type=«ls 2:RootDocumentType»/>
</xsd:sequence>
</xsd:complexType>
</xsd:element>
<xsd:element name=«sendSignal»>
<xsd:complexType>
<xsd:sequence>
<xsd:elementname- «Signal» type=«sgn:Signal»/>
</xsd:sequence>
</xsd:complexTypc>
</xsd:element>
<xsd:element name=«sendResult»>
<xsd:complexType>
<xsd:sequence>
<xsd:element name=«ls_3RootDocnment» type=«ls_3:RootDocumentType»/>
</xsd:sequence>
</xsd:complexType>
</xsd:element>
</xsd:schema>
</wsdl:types>
<wsdl:message name=«sendCertificatcDetails»>
<wsdl:parl name- «parameters» element=«tns:sendCertificateDetails»/>
</wsdl:message>
<wsdl:message name=«sendRequestCertificateDetails»>
<wsdl:part name=«parameters» element=«tns:sendRequestCertificateDetails»/>
</wsdl:message>
<wsdl:message name=«sendResultCertificateDetails»>
<wsdl:part name=«parameters» element=«tns:sendResultCertificateDetails»/>
</wsdl:message>
<wsdl:message name- «sendSignal»>
<wsdl:part name- «parameters» element=«tns:sendSignal»7>
</wsdl:message>
<wsdl:message name=«sendResult»>
<wsdl:part name=«parameters» element=«tns:sendResult»/>
</wsdl:message>
<wsdl:portType name-»EECVNCertificateService_PortType»>
<wsdl:operation name=«sendCertificateDetails»>
<wsdl:documentation>”Providing information on the issued certificate of origin”
service</wsdl:documentation>
<wsdl:input name=«sendCertificateDetails» message=«tns:sendCertificateDetails»
wsam:Action=«http://tempuri.org/EECVNCertificateService/sendCcrtificateDetails«/>
</wsdl:operation>
<wsdl:operation name=«sendRequestCertificateDetails»>
<wsdl:documentation> «Receiving information about the certificate of origin»
service</wsdl:documentation>
<wsdl:input name=«sendRequestCertificateDetails»
message=«tns:sendRequestCertificatcDetails»
wsam:Action=«http://tempuri.org/EECVNCertificateService/sendRequestCertificateDetails«/>
</wsdl:operation>
<wsdl:operation name=«sendResultCertificateDetails»>
<wsdl:documentation> «Receiving results of processing containing information on the certificate
of origin» service</wsdl:documentation>
<wsdl:input name=«sendRcsultCertificateDetails» message- «tns:sendResultCertificateDetails»
wsam:Action=«http://tempuri.org/EECVNCertificateService/sendResultCertificateDetails«/>
</wsdl:operation>
<wsdl:operation name=«sendSignal»>
<wsdl:documentation> «Recciving of signals on the current processing status»
service</wsdl:documentation>
<wsdl:input name- «sendSignal» message=«tns:sendSignal»
wsam:Action=«http://tempuri.org/EECVNCertificateService/sendSignal7>
</wsdl:operation>
<wsdl:operation name=«sendResult»>
<wsdl:documentation>”Receiving of the processing result” service</wsdl:documentation>
<wsdl:input name- «sendResult» message=«tns:sendResult»
wsam:Action=«http://tempuri.org/EECVNCertificateService/sendResult«/>
</wsdl:operation>
</wsdl:portType>
<wsdl:binding name=«EECVNCertificateService_Binding»
type=«tns:EECVNCertificateServiceJPortType»>
<soapl 2:binding style- «document» transport=«http://schemas.xmlsoap.org/soap/http«/>
<wsdl:operation name=«sendCertificateDctails»>
<soap12:operation soapActionRequired=«false» style=«document»/>
<wsdl:input name=«sendCertificateDetails»>
<soapl 2:body use=«literal»7>
</wsdl:input>
</wsdl:operation>
<wsdl:operation name=«sendRequestCertificateDetails»>
<soapl 2:operation soapActionRequired- «false» style=«document»/>
<wsdl:input name=«sendRequestCertificateDetails»>
<soapl 2:body use=«literal»/>
</wsdl:input>
</wsdl:operation>
<wsdl:operation name=«sendResultCertificateDetails»>
<soap12:operation soapActionRequired=«false» style=«document»/>
<wsdl:input name=«sendResultCertificateDetails»>
<soapl 2:body use=«literaI»/>
</wsdl:input>
</wsdl:operation>
<wsdl:operation name- «sendSignal»>
<soapl 2:operation soapActionRequired=«false» style=«document»/>
<wsdl:input name=«sendSignal»>
<soapl 2:body use=«literal»/>
</wsdl:input>
</wsdl:operation>
<wsdl:operation name=«sendResult»>
<soapl 2:operation soapActionRequired=«false» style=«document»/>
<wsdl:input name- «sendResult»>
<soapl 2:body use=«literal»/>
</wsdl:input>
</wsdl:operation>
</wsdl:binding>
<wsdl:service name=«EECVNCertificateService»>
<wsdl:port name=«EECVNCertificateService»
binding=«tns:EECVNCertificateService_Binding»>
<soapl 2:address location=«http://tempuri.org/EECVNCertificateService«/>
</wsdl:port>
</wsdl:service>
</wsdl:definitions>
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